// ===================================================================
// Title:       Application MOF Specification 2.7, BIOS and 
//              Device Driver Software
// Filename:    Application27_BIOS.mof
// Version:     2.7.0
// Status:      Final
// Date:        31 March 2003 
// CVS:         $Revision: 1.2 $           
// ===================================================================
// Copyright 1998-2003 Distributed Management Task Force, Inc. (DMTF).
// All rights reserved.  
// DMTF is a not-for-profit association of industry members dedicated 
// to promoting enterprise and systems management and interoperability. 
// DMTF specifications and documents may be reproduced for uses
// consistent with this purpose by members and non-members, 
// provided that correct attribution is given. 
// As DMTF specifications may be revised from time to time, 
// the particular version and release date should always be noted.
//
// Implementation of certain elements of this standard or proposed 
// standard may be subject to third party patent rights, including 
// provisional patent rights (herein "patent rights"). DMTF makes 
// no representations to users of the standard as to the existence 
// of such rights, and is not responsible to recognize, disclose, or
// identify any or all such third party patent right, owners or 
// claimants, nor for any incomplete or inaccurate identification or 
// disclosure of such rights, owners or claimants. DMTF shall have no 
// liability to any party, in any manner or circumstance, under any 
// legal theory whatsoever, for failure to recognize, disclose, or 
// identify any such third party patent rights, or for such party's
// reliance on the standard or incorporation thereof in its product, 
// protocols or testing procedures. DMTF shall have no liability to 
// any party implementing such standard, whether such implementation 
// is foreseeable or not, nor to any patent owner or claimant, and shall 
// have no liability or responsibility for costs or losses incurred if 
// a standard is withdrawn or modified after publication, and shall be
// indemnified and held harmless by any party implementing the 
// standard from any and all claims of infringement by a patent owner 
// for such implementations.
//
// For information about patents held by third-parties which have 
// notified the DMTF that, in their opinion, such patent may relate to 
// or impact implementations of DMTF standards, visit 
// http://www.dmtf.org/about/policies/disclosures.php.
// ===================================================================
// Description: These classes represent BIOS and device driver-related
//      objects inherited from SoftwareElements and SoftwareFeatures.   
//      They are maintained as a separate MOF file in the 
//      Application Model.
//
//      The object classes below are listed in an order that
//      avoids forward references. Required objects, defined 
//      by other working groups, are omitted.
// ==================================================================
// Change Log for v2.7
//      06/06/2002 CIM 2.7 Preliminary
//         - These BIOS classes are grouped with the Application Model
//               since they inherit from SoftwareElement/Feature
//         - CR718 - Promote SystemBIOS.GroupComponent from 
//              System to ComputerSystem
//      -3/17/2003 CIM 2.7 Final
//         - No Changes
// ===================================================================

#pragma locale ("en_US")



// ===================================================================
// BIOSFeature
// ===================================================================
   [Version ("2.6.0"), Description (
     "BIOSFeature represents the capabilities of the low-level "
     "software that is used to bring up and configure a Computer"
     "System.") ]
class CIM_BIOSFeature : CIM_SoftwareFeature {

      [Description (
        "An array of integers that specify the features "
        "supported by the BIOS. For example, one can specify that "
        "PnP capabilities are provided (value=9) or that infrared "
        "devices are supported (21). Values specified in the "
        "enumeration are taken from both DMI and SMBIOS (the Type 0 "
        "structure, the BIOS Characteristics and BIOS "
        "Characteristics Extension Bytes attributes."),
       ValueMap {"1", "2", "3", "4", "5", "6", "7", "8", "9", 
                 "10", "11", "12", "13", "14", "15", "16", "17", "18", 
                 "19", "20", "21", "22", "23", "24", "25", "26", 
                 "27", "28", "29", "30", "31", "160"},
       Values {"Other", "Unknown", "Undefined", "ISA Support", 
               "MCA Support", "EISA Support", "PCI Support", 
               "PCMCIA Support", "PnP Support", "APM Support", 
               "Upgradeable BIOS", "BIOS Shadowing Allowed", 
               "VL VESA Support", "ESCD Support", 
               "LS-120 Boot Support", "ACPI Support", 
               "I2O Boot Support", "USB Legacy Support", 
               "AGP Support", "PC Card", "IR", "1394", "I2C", 
               "Smart Battery", "ATAPI ZIP Drive Boot Support", 
               "1394 Boot Support", "Boot from CD", 
               "Selectable Boot", "BIOS ROM is Socketed", 
               "Boot from PCMCIA", "EDD Specification Support", 
               "PC-98"},
       MappingStrings {"MIF.DMTF|BIOS Characteristic|004.3"},
       ArrayType ("Indexed"),
       ModelCorrespondence {
        "CIM_BIOSFeature.CharacteristicDescriptions"} ]
   uint16 Characteristics[];

      [Description (
        "An array of free-form strings providing more detailed "
        "explanations for any of the BIOS features indicated in the "
        "Characteristics array. Note, each entry of this array "
        "is related to the entry in the Characteristics array that "
        "is located at the same index."),
       ArrayType ("Indexed"),
       MappingStrings {"MIF.DMTF|BIOS Characteristic|004.4"},
       ModelCorrespondence {"CIM_BIOSFeature.Characteristics"} ]
   string CharacteristicDescriptions[];
};

 
// ===================================================================
// BIOSElement
// ===================================================================
   [Version ("2.6.0"), Description (
     "BIOSElement represents the low-level software that is loaded "
     "into non-volatile storage and used to bring up and configure "
     "a ComputerSystem.") ]
class CIM_BIOSElement : CIM_SoftwareElement {

      [Override ("Version"),
       MappingStrings {"MIF.DMTF|System BIOS|001.3"} ]
   string Version;

      [Override ("Manufacturer"),
       MappingStrings {"MIF.DMTF|System BIOS|001.2"} ]
   string Manufacturer;   
  
      [Description (
      "If true, this is the primary BIOS of the ComputerSystem."),
       MappingStrings {"MIF.DMTF|System BIOS|001.9"} ]
   boolean PrimaryBIOS;

      [Description (
        "A list of installable languages for the BIOS. This "
        "information can be obtained from SMBIOS, from the string list "
        "that follows the Type 13 structure. An ISO 639 Language Name "
        "should be used to specify the BIOS' installable languages. "
        "The ISO 3166 Territory Name and the encoding method may also "
        "be specified, following the Language Name.") ]
   string ListOfLanguages[];

      [Description (
        "The currently selected language for the BIOS. This "
        "information can be obtained from SMBIOS, using the Current "
        "Language attribute of the Type 13 structure, to index into "
        "the string list following the structure. The property is "
        "formatted using the ISO 639 Language Name, and may be "
        "followed by the ISO 3166 Territory Name and the encoding "
        "method."),
       ModelCorrespondence {"CIM_BIOSElement.ListOfLanguages"} ]
   string CurrentLanguage;

      [Description (
        "The starting address of the memory which this BIOS "
        "occupies."), 
       MappingStrings {"MIF.DMTF|System BIOS|001.5"} ]
    uint64 LoadedStartingAddress;

      [Description (
        "The ending address of the memory which this BIOS "
        "occupies."),
       MappingStrings {"MIF.DMTF|System BIOS|001.6"} ]
    uint64 LoadedEndingAddress;

      [MaxLen (64), Description (
        "A free form string describing the BIOS flash/load utility "
        "that is required to update the BIOSElement. Version and "
        "other information may be indicated in this property."),
       MappingStrings {"MIF.DMTF|System BIOS|001.7"} ]
    string LoadUtilityInformation;

      [Description (
        "Date that this BIOS was released."),
       MappingStrings {"MIF.DMTF|System BIOS|001.8"} ]
    datetime ReleaseDate;
};


// ===================================================================
// BIOSFeatureBIOSElements
// ===================================================================
   [Association, Aggregation, Version ("2.6.0"), Description (
      "A link between BIOSFeature and its aggregated BIOSElements.") ]
class CIM_BIOSFeatureBIOSElements : 
 CIM_SoftwareFeatureSoftwareElements {

      [Override ("GroupComponent"), Aggregate, 
       Description ("The BIOSFeature.") ]
   CIM_BIOSFeature REF GroupComponent;

      [Override ("PartComponent"),
       Description (
        "The BIOSElement that implements the capabilities described "
        "by BIOSFeature.") ]
   CIM_BIOSElement REF PartComponent;
};


// ===================================================================
// SystemBIOS
// ===================================================================
[Association, Aggregation, Version ("2.7.0"), Description (
     "SystemBIOS associates a UnitaryComputerSystem's BIOS with the "
     "System itself.") ]
class CIM_SystemBIOS : CIM_SystemComponent {

      [Override ("GroupComponent"), Max (1), Aggregate, 
       Description (
        "The ComputerSystem that boots from the BIOS.") ]
   CIM_ComputerSystem REF GroupComponent;

      [Override ("PartComponent"), 
       Description ("The System's BIOS.") ]
   CIM_BIOSElement REF PartComponent;
};


// ===================================================================
// VideoBIOSFeature
// ===================================================================
[Version ("2.6.0"), Description (
   "VideoBIOSFeature represents the capabilities of the low-level "
   "software that is used to bring up, configure and use a "
   "ComputerSystem's VideoController and Display.") ] 
class CIM_VideoBIOSFeature : CIM_SoftwareFeature {

   [Description (
       "An array of integers that specify the features supported by "
       "the VideoBIOS. For example, one could indicate support for "
       "VESA power management (value=6) or video BIOS shadowing (8). "
       "The value, 3, is not valid in the CIM Schema since in DMI it "
       "represents that no BIOS Features are supported.  In this "
       "case, the object should not be instantiated."),
    ValueMap {"1", "2", "3", "4", "5", "6", "7", "8", "9"},
    Values {"Other", "Unknown", "Undefined", "Standard Video BIOS",
       "VESA BIOS Extensions Supported", 
       "VESA Power Management Supported", 
       "VESA Display Data Channel Supported", 
       "Video BIOS Shadowing Allowed", "Video BIOS Upgradeable"},
    ArrayType ("Indexed"), 
    MappingStrings {"MIF.DMTF|Video BIOS Characteristic|001.3"},
    ModelCorrespondence {
       "CIM_VideoBIOSFeature.CharacteristicDescriptions"} ]
   uint16 Characteristics[];

   [Description (
       "An array of free-form strings providing more detailed "
       "explanations for any of the VideoBIOS features indicated in "
       "the Characteristics array. Note, each entry of this array "
       "is related to the entry in the Characteristics array that "
       "is located at the same index."),
    ArrayType ("Indexed"),
    MappingStrings {"MIF.DMTF|Video BIOS Characteristic|001.4"},
    ModelCorrespondence {"CIM_VideoBIOSFeature.Characteristics"} ]
   string CharacteristicDescriptions[];
};


// ===================================================================
// VideoBIOSElement
// ===================================================================
[Version ("2.6.0"), Description (
   "VideoBIOSElement represents the low-level software that is "
   "loaded into non-volatile storage and used to bring up, "
   "configure and access a ComputerSystem's VideoController and "
   "Display.") ] 
class CIM_VideoBIOSElement : CIM_SoftwareElement {

   [Override ("Version"),
    MappingStrings {"MIF.DMTF|Video BIOS|001.3"} ]
   string Version;

   [Override ("Manufacturer"),
    MappingStrings {"MIF.DMTF|Video BIOS|001.2"} ]
   string Manufacturer; 

   [Description (
       "If true, indicates that the Video BIOS is shadowed."),
    MappingStrings {"MIF.DMTF|Video BIOS|001.5"} ]
   boolean IsShadowed;

   [Description (
       "Date that this BIOS was released."),
    MappingStrings {"MIF.DMTF|Video BIOS|001.4"} ]
   datetime ReleaseDate;
};


// ===================================================================
// VideoBIOSFeatureVideoBIOSElements
// ===================================================================
[Association, Aggregation, Version ("2.6.0"), Description (
   "A link between VideoBIOSFeature and its aggregated "
   "VideoBIOSElements.") ] 
class CIM_VideoBIOSFeatureVideoBIOSElements : 
 CIM_SoftwareFeatureSoftwareElements {

   [Override ("GroupComponent"), Aggregate,
    Description ("The VideoBIOSFeature.") ]
   CIM_VideoBIOSFeature REF GroupComponent;

   [Override ("PartComponent"),
    Description (
       "The VideoBIOSElement that implements the capabilities "
       "described by VideoBIOSFeature.") ]
   CIM_VideoBIOSElement REF PartComponent;
};


// ===================================================================
// AGPSoftwareFeature
// ===================================================================
[Version ("2.6.0"), Description (
   "AGPSoftwareFeature adds two attributes to SoftwareFeature "
   "to represent the capabilities of an AGP device driver. An "
   "instance of this class would be associated with the "
   "Driver's SoftwareElement using the SoftwareFeatureSoftware"
   "Elements relationship. The driver's SoftwareElement is "
   "associated with the AGPVideoController via the Device"
   "Software relationship.") ]
class CIM_AGPSoftwareFeature : CIM_SoftwareFeature {

   [Description (
       "An array of integers indicating various capabilities and "
       "characteristics of the AGPVideoController."), 
    ArrayType ("Indexed"), 
    ValueMap {"0", "1", "2", "3", "4", "5", "6"},
    Values {"Unknown", "Other", "OS support", 
       "Hardware Acceleration", "Hardware Blit", 
       "OpenGL Support", "Cache Coherency"}, 
    ModelCorrespondence {
       "CIM_AGPSoftwareFeature.CharacteristicDescriptions"} ]
   uint16 Characteristics[];

   [Description (
       "An array of free-form strings providing more detailed "
       "explanations for any of the features indicated in the "
       "Characteristics array. Each entry in this array is "
       "related to the Characteristics array entry located at "
       "the same index."), 
    ArrayType ("Indexed"), 
    ModelCorrespondence {"CIM_AGPSoftwareFeature.Characteristics"} ]
   string CharacteristicDescriptions[];
};


// ==================================================================
// end of file
// ==================================================================
