// ===================================================================
// Title:       Core Settings 2.8
// Filename:    Core28_Settings.mof
// Version:     2.8
// Status:      Final
// Date:        Jan 26, 2004
// ===================================================================
// Copyright 1999-2003 Distributed Management Task Force, Inc. (DMTF).
// All rights reserved.
// DMTF is a not-for-profit association of industry members dedicated
// to promoting enterprise and systems management and interoperability.
// DMTF specifications and documents may be reproduced for uses
// consistent with this purpose by members and non-members,
// provided that correct attribution is given.
// As DMTF specifications may be revised from time to time,
// the particular version and release date should always be noted.
// 
// Implementation of certain elements of this standard or proposed
// standard may be subject to third party patent rights, including
// provisional patent rights (herein "patent rights"). DMTF makes
// no representations to users of the standard as to the existence
// of such rights, and is not responsible to recognize, disclose, or
// identify any or all such third party patent right, owners or
// claimants, nor for any incomplete or inaccurate identification or
// disclosure of such rights, owners or claimants. DMTF shall have no
// liability to any party, in any manner or circumstance, under any
// legal theory whatsoever, for failure to recognize, disclose, or
// identify any such third party patent rights, or for such party's
// reliance on the standard or incorporation thereof in its product,
// protocols or testing procedures. DMTF shall have no liability to
// any party implementing such standard, whether such implementation
// is foreseeable or not, nor to any patent owner or claimant, and shall
// have no liability or responsibility for costs or losses incurred if
// a standard is withdrawn or modified after publication, and shall be
// indemnified and held harmless by any party implementing the
// standard from any and all claims of infringement by a patent owner
// for such implementations.
// 
// For information about patents held by third-parties which have
// notified the DMTF that, in their opinion, such patent may relate to
// or impact implementations of DMTF standards, visit
// http://www.dmtf.org/about/policies/disclosures.php.
// ===================================================================
// Description: The Core Model defines basic management concepts.
//              This file defines Settings/SettingData and their
//              groupings, Profiles and Configurations.
// 
//              The object classes below are listed in an order that
//              avoids forward references. Required objects, defined
//              by other working groups, are omitted.
// ==================================================================
// Change Log for v2.8 Final
// CR1128  - Addition of HostedDependency
// CR1223 - SysDev Omnibus CR - Minor MOF corrections.
// 
// Change Log for v2.7 Final
// CR927 - Relax cardinality for the ManagedElement side of
// ElementProfile
//       - Update the description of Profile to reflect this change.
// CR968 - Remove the Experimental qualifier
// CR994 - Update description of InstanceID
// 
// Change Log for v2.7
// CR723 - Introduce SettingData, ScopedSetttingData, ScopedSetting,
//         and ElementSettingData.
//       - Clarify the description of Setting to reconcile with
//         SettingData.
// CR642 - Add Profile and ElementProfile
// ==================================================================

#pragma locale ("en_US")


// ===================================================================
// SettingData
// ===================================================================
   [Abstract, Version ( "2.7.0" ), Description (
       "The SettingData class represents configuration-related and "
       "operational parameters for one or more ManagedElement(s). A "
       "ManagedElement may have multiple SettingData objects "
       "associated with it. The current operational values for an "
       "Element's parameters are reflected by properties in the "
       "Element itself or by properties in its associations. These "
       "properties do not have to be the same values present in the "
       "SettingData object. For example, a modem may have a "
       "SettingData baud rate of 56Kb/sec but be operating at "
       "19.2Kb/sec. \n"
       "Note that the CIM_SettingData class is very similar to "
       "CIM_Setting, yet both classes are present in the model. This "
       "is because many implementations have successfully used "
       "CIM_Setting. However, issues have arisen that could not be "
       "resolved without defining a new class. Therefore, until a new "
       "major release occurs, both classes will exist in the model. "
       "Refer to the Core White Paper for additional information.")]
class CIM_SettingData : CIM_ManagedElement {

      [Key, Description (
          "Within the scope of the instantiating Namespace, InstanceID "
          "opaquely and uniquely identifies an instance of this class. "
          "In order to ensure uniqueness within the NameSpace, the "
          "value of InstanceID SHOULD be constructed using the "
          "following 'preferred' algorithm: \n"
          "<OrgID>:<LocalID> \n"
          "Where <OrgID> and <LocalID> are separated by a colon ':', "
          "and where <OrgID> MUST include a copyrighted, trademarked "
          "or otherwise unique name that is owned by the business "
          "entity creating/defining the InstanceID, or is a registered "
          "ID that is assigned to the business entity by a recognized "
          "global authority (This is similar to the <Schema "
          "Name>_<Class Name> structure of Schema class names.) In "
          "addition, to ensure uniqueness <OrgID> MUST NOT contain a "
          "colon (':'). When using this algorithm, the first colon to "
          "appear in InstanceID MUST appear between <OrgID> and "
          "<LocalID>. \n"
          "<LocalID> is chosen by the business entity and SHOULD not "
          "be re-used to identify different underlying (real-world) "
          "elements. If the above 'preferred' algorithm is not used, "
          "the defining entity MUST assure that the resultant "
          "InstanceID is not re-used across any InstanceIDs produced "
          "by this or other providers for this instance's NameSpace. \n"
          "For DMTF defined instances, the 'preferred' algorithm MUST "
          "be used with the <OrgID> set to 'CIM'.")]
   string InstanceID;

      [Required, Override ( "ElementName" ), Description (
          "The user friendly name for this instance of SettingData. In "
          "addition, the user friendly name can be used as a index "
          "property for a search of query. (Note: Name does not have "
          "to be unique within a namespace.)")]
   string ElementName;
};


// ===================================================================
// ScopedSettingData
// ===================================================================
   [Abstract, Version ( "2.7.0" ), Description (
       "The ScopedSettingData class represents the general concept of "
       "SettingData which is scoped/contained by a ManagedElement "
       "(i.e. settings that are specifically defined for a system, "
       "device, etc). ScopedSettingData is tied to a ManagedElement "
       "using the ScopedSetting association. Note that the cardinality "
       "of the ManagedElement reference is Min(1), Max(1). This "
       "cardinality mandates the instantiation of the ScopedSetting "
       "association for the referenced instance of ScopedSettingData. "
       "ScopedSetting describes the existence requirements and context "
       "for the referenced instance of ManagedElement. Specifically, "
       "the ManagedElement MUST exist and provides the context for the "
       "ScopedSettingData.")]
class CIM_ScopedSettingData : CIM_SettingData {
};


// ===================================================================
// ScopedSetting
// ===================================================================
   [Association, Version ( "2.8.0" ), Description (
       "ScopedSetting defines a setting in the context of the Managed "
       "Element which it resides.")]
class CIM_ScopedSetting : CIM_HostedDependency {

      [Override ( "Antecedent" ), Min ( 1 ), Max ( 1 ), Description (
          "The scoping ManagedElement.")]
   CIM_ManagedElement REF Antecedent;

      [Override ( "Dependent" ), Description (
          "The setting defined for the ManagedElement.")]
   CIM_ScopedSettingData REF Dependent;
};


// ===================================================================
// ElementSettingData
// ===================================================================
   [Association, Version ( "2.7.0" ), Description (
       "ElementSettingData represents the association between "
       "ManagedElements and applicable setting data. This association "
       "also describes whether this is a default or current setting.")]
class CIM_ElementSettingData {

      [Key, Description (
          "The managed element.")]
   CIM_ManagedElement REF ManagedElement;

      [Key, Description (
          "The SettingData object associated with the element.")]
   CIM_SettingData REF SettingData;

      [Description (
          "An enumerated integer indicating that the referenced "
          "setting is a default setting for the element, or that this "
          "information is unknown."), 
       ValueMap { "0", "1", "2" }, 
       Values { "Unknown", "Is Default", "Is Not Default" }]
   uint16 IsDefault;

      [Description (
          "An enumerated integer indicating that the referenced "
          "setting is currently being used in the operation of the "
          "element, or that this information is unknown."), 
       ValueMap { "0", "1", "2" }, 
       Values { "Unknown", "Is Current", "Is Not Current" }]
   uint16 IsCurrent;
};


// ==================================================================
// Profile
// ==================================================================
   [Version ( "2.7.0" ), Description (
       "Profile specifies a general collection of Settings/SettingData "
       "that are logically grouped together. Note that the CIM_Profile "
       "class uses simplified naming/identity and collection "
       "algorithms, as compared to CIM_Configuration. The settings are "
       "'collected' into the Profile using the MemberOfCollection "
       "association. Note that a Profile obtains its setting data and "
       "other necessary information from collected Setting/SettingData "
       "instances, and by the definition of additional properties in "
       "subclasses. One example of a Profile is to define the "
       "collection of settings for a particular person. Another is to "
       "define the collection of settings appropriate when "
       "initializing a system. \n"
       "\n"
       "Profile is tied to a ManagedElement using the ElementProfile "
       "association. The ManagedElement provides context for the "
       "Profile, and the settings collected by Profile SHOULD be "
       "settings of the associated ManagedElement. Note that a "
       "ManagedElement MAY NOT exist when the Profile is instantiated. "
       "This is true when the Profile is used in the creation of the "
       "real world entity represented by (and then instantiated in) "
       "the ManagedElement.")]
class CIM_Profile : CIM_Collection {

      [Key, Description (
          "Within the scope of the instantiating Namespace, InstanceID "
          "opaquely and uniquely identifies an instance of this class. "
          "In order to ensure uniqueness within the NameSpace, the "
          "value of InstanceID SHOULD be constructed using the "
          "following 'preferred' algorithm: \n"
          "<OrgID>:<LocalID> \n"
          "Where <OrgID> and <LocalID> are separated by a colon ':', "
          "and where <OrgID> MUST include a copyrighted, trademarked "
          "or otherwise unique name that is owned by the business "
          "entity creating/defining the InstanceID, or is a registered "
          "ID that is assigned to the business entity by a recognized "
          "global authority (This is similar to the <Schema "
          "Name>_<Class Name> structure of Schema class names.) In "
          "addition, to ensure uniqueness <OrgID> MUST NOT contain a "
          "colon (':'). When using this algorithm, the first colon to "
          "appear in InstanceID MUST appear between <OrgID> and "
          "<LocalID>. \n"
          "<LocalID> is chosen by the business entity and SHOULD not "
          "be re-used to identify different underlying (real-world) "
          "elements. If the above 'preferred' algorithm is not used, "
          "the defining entity MUST assure that the resultant "
          "InstanceID is not re-used across any InstanceIDs produced "
          "by this or other providers for this instance's NameSpace. \n"
          "For DMTF defined instances, the 'preferred' algorithm MUST "
          "be used with the <OrgID> set to 'CIM'.")]
   string InstanceID;
};


// ===================================================================
// ElementProfile
// ===================================================================
   [Association, Version ( "2.7.0" ), Description (
       "ElementProfile represents the association between "
       "ManagedElements and the Profiles (collection of settings) "
       "defined for them. This association describes that the settings "
       "collected by the Profile apply to the associated "
       "ManagedElement.")]
class CIM_ElementProfile {

      [Key, Description (
          "The managed element.")]
   CIM_ManagedElement REF ManagedElement;

      [Key, Description (
          "The Profile object associated with the element.")]
   CIM_Profile REF Profile;
};


// ===================================================================
// Setting
// ===================================================================
   [Abstract, Version ( "2.7.0" ), Description (
       "The Setting class represents configuration-related and "
       "operational parameters for one or more "
       "ManagedSystemElement(s). An Element may have multiple Setting "
       "objects associated with it. The current operational values for "
       "an Element's parameters are reflected by properties in the "
       "Element itself or by properties in its associations. These "
       "properties do not have to be the same values present in the "
       "Setting object. For example, a modem may have a Setting baud "
       "rate of 56Kb/sec but be operating at 19.2Kb/sec. \n"
       "Note that the CIM_SettingData class is very similar to "
       "CIM_Setting, yet both classes are present in the model. This "
       "is because many implementations have successfully used "
       "CIM_Setting. However, issues have arisen that could not be "
       "resolved without defining a new class. Therefore, until a new "
       "major release occurs, both classes will exist in the model. "
       "Refer to the Core White Paper for additional information.")]
class CIM_Setting : CIM_ManagedElement {

      [Description (
          "The identifier by which the Setting object is known."), 
       MaxLen ( 256 )]
   string SettingID;

      [Description (
          "The VerifyOKToApplyToMSE method is used to verify that this "
          "Setting can be 'applied' to the referenced Managed "
          "SystemElement, at the given time or time interval. This "
          "method takes three input parameters: MSE (the Managed "
          "SystemElement that is being verified), TimeToApply (which, "
          "being a datetime, can be either a specific time or a time "
          "interval), and MustBeCompletedBy (which indicates the "
          "required completion time for the method). The return value "
          "should be 0 if it is OK to apply the Setting, 1 if the "
          "method is not supported, 2 if the Setting cannot be applied "
          "within the specified times, and any other number if an "
          "error occurred. In a subclass, the set of possible return "
          "codes could be specified, using a ValueMap qualifier on the "
          "method. The strings to which the ValueMap contents are "
          "'translated' may also be specified in the subclass as a "
          "Values array qualifier.")]
   uint32 VerifyOKToApplyToMSE( 
         [IN, Description (
             "The Managed SystemElement that is being verified.")]
      CIM_ManagedSystemElement REF MSE, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy); 

      [Description (
          "The ApplyToMSE method performs the actual application of "
          "the Setting to the referenced ManagedSystemElement. It "
          "takes three input parameters: MSE (the ManagedSystem "
          "Element to which the Setting is being applied), TimeToApply "
          "(which, being a datetime, can be either a specific time or "
          "a time interval), and MustBeCompletedBy (which indicates "
          "the required completion time for the method). Note that the "
          "semantics of this method are that individual Settings are "
          "either wholly applied or not applied at all to their target "
          "ManagedSystemElement. The return value should be 0 if the "
          "Setting is successfully applied to the referenced "
          "ManagedSystemElement, 1 if the method is not supported, 2 "
          "if the Setting was not applied within the specified times, "
          "and any other number if an error occurred. In a subclass, "
          "the set of possible return codes could be specified, using "
          "a ValueMap qualifier on the method. The strings to which "
          "the ValueMap contents are 'translated' may also be "
          "specified in the subclass as a Values array qualifier. \n"
          "Note: If an error occurs in applying the Setting to a "
          "ManagedSystemElement, the Element must be configured as "
          "when the 'Apply' attempt began. That is, the Element should "
          "NOT be left in an indeterminate state.")]
   uint32 ApplyToMSE( 
         [IN, Description (
             "The ManagedSystem Element to which the Setting is being "
             "applied.")]
      CIM_ManagedSystemElement REF MSE, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy); 

      [Description (
          "The VerifyOKToApplyToCollection method is used to verify "
          "that this Setting can be 'applied' to the referenced "
          "Collection of ManagedSystemElements, at the given time or "
          "time interval, without causing adverse effects to either "
          "the Collection itself or its surrounding environment. The "
          "net effect is to execute the VerifyOKToApply method against "
          "each of the Elements aggregated by the Collection. This "
          "method takes three input parameters: Collection (the "
          "Collection of Managed SystemElements that is being "
          "verified), TimeToApply (which, being a datetime, can be "
          "either a specific time or a time interval), and "
          "MustBeCompletedBy (which indicates the required completion "
          "time for the method). The return value should be 0 if it is "
          "OK to apply the Setting, 1 if the method is not supported, "
          "2 if the Setting cannot be applied within the specified "
          "times, and any other number if an error occurred. One "
          "output parameter is defined - CanNotApply - which is a "
          "string array that lists the keys of the "
          "ManagedSystemElements to which the Setting can NOT be "
          "applied. This enables those Elements to be revisited and "
          "either fixed, or other corrective action taken. \n"
          "In a subclass, the set of possible return codes could be "
          "specified, using a ValueMap qualifier on the method. The "
          "strings to which the ValueMap contents are 'translated' may "
          "also be specified in the subclass as a Values array "
          "qualifier.")]
   uint32 VerifyOKToApplyToCollection ( 
         [IN, Description (
             "The Collection of Managed SystemElements that is being "
             "verified.")]
      CIM_CollectionOfMSEs REF Collection, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy, 
         [IN ( false ), OUT, Description (
             "A string array that lists the keys of the "
             "ManagedSystemElements to which the Setting can NOT be "
             "applied.")]
      string CanNotApply[]); 

      [Description (
          "The ApplyToCollection method performs the application of "
          "the Setting to the referenced Collection of ManagedSystem "
          "Elements. The net effect is to execute the ApplyToMSE "
          "method against each of the Elements aggregated by the "
          "Collection. If the input value ContinueOnError is FALSE, "
          "this method applies the Setting to all Elements in the "
          "Collection until it encounters an error, in which case it "
          "stops execution, logs the key of the Element that caused "
          "the error in the CanNotApply array, and issues a return "
          "code of 2. If the input value ContinueOnError is TRUE, then "
          "this method applies the Setting to all the "
          "ManagedSystemElements in the Collection, and reports the "
          "failed Elements in the array, CanNotApply. For the latter, "
          "processing will continue until the method is applied to all "
          "Elements in the Collection, regardless of any errors "
          "encountered. The key of each ManagedSystemElement to which "
          "the Setting could not be applied is logged into the "
          "CanNotApply array. This method takes four input parameters: "
          "Collection (the Collection of Elements to which the Setting "
          "is being applied), TimeToApply (which, being a datetime, "
          "can be either a specific time or a time interval), "
          "ContinueOnError (TRUE means to continue processing on "
          "encountering an error), and MustBeCompletedBy (which "
          "indicates the required completion time for the method). The "
          "return value should be 0 if the Setting is successfully "
          "applied to the referenced Collection, 1 if the method is "
          "not supported, 2 if the Setting was not applied within the "
          "specified times, 3 if the Setting cannot be applied using "
          "the input value for ContinueOnError, and any other number "
          "if an error occurred. One output parameter is defined, "
          "CanNotApplystring, which is an array that lists the keys of "
          "the ManagedSystemElements to which the Setting was NOT able "
          "to be applied. This output parameter has meaning only when "
          "the ContinueOnError parameter is TRUE. \n"
          "In a subclass, the set of possible return codes could be "
          "specified, using a ValueMap qualifier on the method. The "
          "strings to which the ValueMap contents are 'translated' may "
          "also be specified in the subclass as a Values array "
          "qualifier. \n"
          "Note: if an error occurs in applying the Setting to a "
          "ManagedSystemElement in the Collection, the Element must be "
          "configured as when the 'Apply' attempt began. That is, the "
          "Element should NOT be left in an indeterminate state.")]
   uint32 ApplyToCollection( 
         [IN, Description (
             "The Collection of Managed SystemElements to be applied.")]
      CIM_CollectionOfMSEs REF Collection, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "TRUE means to continue processing on encountering an "
             "error.")]
      boolean ContinueOnError, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy, 
         [IN ( false ), OUT, Description (
             "A string array that lists the keys of the "
             "ManagedSystemElements to which the Setting was NOT be "
             "applied.")]
      string CanNotApply[]); 

      [Description (
          "The VerifyOKToApplyIncrementalChangeToMSE method is used to "
          "verify that a subset of the properties in this Setting can "
          "be 'applied' to the referenced Managed SystemElement, at "
          "the given time or time interval. This method takes four "
          "input parameters: MSE (the Managed SystemElement that is "
          "being verified), TimeToApply (which, being a datetime, can "
          "be either a specific time or a time interval), "
          "MustBeCompletedBy (which indicates the required completion "
          "time for the method), and a PropertiesToApply array (which "
          "contains a list of the property names whose values will be "
          "verified.) If the array is null, empty or contains the "
          "string \"ALL\" as a property name, then all Settings "
          "properties shall be verified. If it is set to \"NONE\", "
          "then no Settings properties will be verified. The return "
          "value should be 0 if it is OK to apply the Setting, 1 if "
          "the method is not supported, 2 if the Setting cannot be "
          "applied within the specified times, and any other number if "
          "an error occurred. In a subclass, the set of possible "
          "return codes could be specified, using a ValueMap qualifier "
          "on the method. The strings to which the ValueMap contents "
          "are 'translated' may also be specified in the subclass as a "
          "Values array qualifier.")]
   uint32 VerifyOKToApplyIncrementalChangeToMSE( 
         [IN, Description (
             "The ManagedSystem Element for which the Setting is being "
             "verified.")]
      CIM_ManagedSystemElement REF MSE, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy, 
         [IN, Description (
             "A list of the property names whose values will be "
             "verified.")]
      string PropertiesToApply[]); 

      [Description (
          "The ApplyIncrementalChangeToMSE method performs the actual "
          "application of a subset of the properties in the Setting to "
          "the referenced ManagedSystemElement. It takes four input "
          "parameters: MSE (the ManagedSystem Element to which the "
          "Setting is being applied), TimeToApply (which, being a "
          "datetime, can be either a specific time or a time "
          "interval), MustBeCompletedBy (which indicates the required "
          "completion time for the method), and a PropertiesToApply "
          "array (which contains a list of the property names whose "
          "values will be applied.) If a property is not in this list, "
          "it will be ignored by the Apply. If the array is null, "
          "empty or contains the string \"ALL\" as a property name, "
          "then all Settings properties shall be applied. If it is set "
          "to \"NONE\", then no Settings properties will be applied. \n"
          "Note that the semantics of this method are that individual "
          "Settings are either wholly applied or not applied at all to "
          "their target ManagedSystemElement. The return value should "
          "be 0 if the Setting is successfully applied to the "
          "referenced ManagedSystemElement, 1 if the method is not "
          "supported, 2 if the Setting was not applied within the "
          "specified times, and any other number if an error occurred. "
          "In a subclass, the set of possible return codes could be "
          "specified, using a ValueMap qualifier on the method. The "
          "strings to which the ValueMap contents are 'translated' may "
          "also be specified in the subclass as a Values array "
          "qualifier. \n"
          "Note: If an error occurs in applying the Setting to a "
          "ManagedSystemElement, the Element must be configured as "
          "when the 'Apply' attempt began. That is, the Element should "
          "NOT be left in an indeterminate state.")]
   uint32 ApplyIncrementalChangeToMSE( 
         [IN, Description (
             "The ManagedSystem Element to which the Setting is being "
             "applied.")]
      CIM_ManagedSystemElement REF MSE, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy, 
         [IN, Description (
             "A list of the property names whose values will be "
             "applied.")]
      string PropertiesToApply[]); 

      [Description (
          "The VerifyOKToApplyIncrementalChangeToCollection method is "
          "used to verify that a subset of the properties in this "
          "Setting can be 'applied' to the referenced Collection of "
          "ManagedSystemElements, at the given time or time interval, "
          "without causing adverse effects to either the Collection "
          "itself or its surrounding environment. The net effect is to "
          "execute the VerifyOKToApplyIncrementalChangeToMSE method "
          "against each of the Elements aggregated by the Collection. "
          "This method takes three input parameters: Collection (the "
          "Collection of Managed SystemElements that is being "
          "verified), TimeToApply (which, being a datetime, can be "
          "either a specific time or a time interval), "
          "MustBeCompletedBy (which indicates the required completion "
          "time for the method), and a PropertiesToApply array (which "
          "contains a list of the property names whose values will be "
          "verified. If they array is null or empty or constains the "
          "string \"all\" as a property name then all Settings "
          "properties shall be verified. If it is set to \"none\" then "
          "no Settings properties will be verified). The return value "
          "should be 0 if it is OK to apply the Setting, 1 if the "
          "method is not supported, 2 if the Setting cannot be applied "
          "within the specified times, and any other number if an "
          "error occurred. One output parameter is defined - "
          "CanNotApply - which is a string array that lists the keys "
          "of the ManagedSystemElements to which the Setting can NOT "
          "be applied. This enables those Elements to be revisited and "
          "either fixed, or other corrective action taken. \n"
          "In a subclass, the set of possible return codes could be "
          "specified, using a ValueMap qualifier on the method. The "
          "strings to which the ValueMap contents are 'translated' may "
          "also be specified in the subclass as a Values array "
          "qualifier.")]
   uint32 VerifyOKToApplyIncrementalChangeToCollection ( 
         [IN, Description (
             "The Collection of Managed SystemElements for which the "
             "setting is being verified.")]
      CIM_CollectionOfMSEs REF Collection, 
         [IN, Description (
             "TimeToApply can be either a specific time or a time "
             "interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "The required completion time for the method.")]
      datetime MustBeCompletedBy, 
         [IN, Description (
             "A list of the property names whose values will be "
             "verified.")]
      string PropertiesToApply[], 
         [IN ( false ), OUT, Description (
             "A string array that lists the keys of the "
             "ManagedSystemElements to which the Setting can NOT be "
             "applied.")]
      string CanNotApply[]); 

      [Description (
          "The ApplyIncrementalChangeToCollection method performs the "
          "application of a subset of the properties in this Setting "
          "to the referenced Collection of ManagedSystem Elements. The "
          "net effect is to execute the ApplyIncrementalChangeToMSE "
          "method against each of the Elements aggregated by the "
          "Collection. If the input value ContinueOnError is FALSE, "
          "this method applies the Setting to all Elements in the "
          "Collection until it encounters an error, in which case it "
          "stops execution, logs the key of the Element that caused "
          "the error in the CanNotApply array, and issues a return "
          "code of 2. If the input value ContinueOnError is TRUE, then "
          "this method applies the Setting to all the "
          "ManagedSystemElements in the Collection, and reports the "
          "failed Elements in the array, CanNotApply. For the latter, "
          "processing will continue until the method is applied to all "
          "Elements in the Collection, regardless of any errors "
          "encountered. The key of each ManagedSystemElement to which "
          "the Setting could not be applied is logged into the "
          "CanNotApply array. This method takes four input parameters: "
          "Collection (the Collection of Elements to which the Setting "
          "is being applied), TimeToApply (which, being a datetime, "
          "can be either a specific time or a time interval), "
          "ContinueOnError (TRUE means to continue processing on "
          "encountering an error), and MustBeCompletedBy (which "
          "indicates the required completion time for the method), and "
          "a PropertiesToApply array (which contains a list of the "
          "property names whose values will be applied.) If a property "
          "is not in this list, it will be ignored by the Apply. If "
          "the array is null or empty or contains the string \"ALL\" "
          "as a property name, then all Settings properties shall be "
          "applied. If it is set to \"NONE\", then no Settings "
          "properties will be applied. \n"
          "The return value should be 0 if the Setting is successfully "
          "applied to the referenced Collection, 1 if the method is "
          "not supported, 2 if the Setting was not applied within the "
          "specified time, 3 if the Setting cannot be applied using "
          "the input value for ContinueOnError, and any other number "
          "if an error occurred. One output parameter is defined, "
          "CanNotApplystring, which is an array that lists the keys of "
          "the ManagedSystemElements to which the Setting was NOT able "
          "to be applied. This output parameter has meaning only when "
          "the ContinueOnError parameter is TRUE. \n"
          "In a subclass, the set of possible return codes could be "
          "specified, using a ValueMap qualifier on the method. The "
          "strings to which the ValueMap contents are 'translated' may "
          "also be specified in the subclass as a Values array "
          "qualifier. \n"
          "Note: if an error occurs in applying the Setting to a "
          "ManagedSystemElement in the Collection, the Element must be "
          "configured as when the 'Apply' attempt began. That is, the "
          "Element should NOT be left in an indeterminate state.")]
   uint32 ApplyIncrementalChangeToCollection( 
         [IN, Description (
             "The Collection of Elements to which the Setting is being "
             "applied.")]
      CIM_CollectionOfMSEs REF Collection, 
         [IN, Description (
             "A specific time or a time interval.")]
      datetime TimeToApply, 
         [IN, Description (
             "TRUE means to continue processing on encountering an "
             "error.")]
      boolean ContinueOnError, 
         [IN, Description (
             "This parameter indicates the required completion time "
             "for the method.")]
      datetime MustBeCompletedBy, 
         [IN, Description (
             "A list of the property names whose values will be "
             "verified.")]
      string PropertiesToApply[], 
         [IN ( false ), OUT, Description (
             "A string array that lists the keys of the "
             "ManagedSystemElements to which the Setting can NOT be "
             "applied.")]
      string CanNotApply[]); 
};


// ===================================================================
// ElementSetting
// ===================================================================
   [Association, Version ( "2.6.0" ), Description (
       "ElementSetting represents the association between Managed "
       "SystemElements and the Setting class(es) defined for them.")]
class CIM_ElementSetting {

      [Key, Description (
          "The ManagedSystemElement.")]
   CIM_ManagedSystemElement REF Element;

      [Key, Description (
          "The Setting object associated with the ManagedSystem "
          "Element.")]
   CIM_Setting REF Setting;
};


// ===================================================================
// DefaultSetting
// ===================================================================
   [Association, Version ( "2.6.0" ), Description (
       "DefaultSetting represents the association between a Managed "
       "SystemElement and the single Setting class that is defined to "
       "be the default setting for this Element.")]
class CIM_DefaultSetting : CIM_ElementSetting {

      [Override ( "Setting" ), Max ( 1 ), Description (
          "The Setting object which is the default.")]
   CIM_Setting REF Setting;
};


// ==================================================================
// CIM_SystemSetting
// ==================================================================
   [Abstract, Version ( "2.6.0" ), Description (
       "CIM_SystemSetting represents the general concept of a "
       "CIM_Setting which is scoped by/weak to a System.")]
class CIM_SystemSetting : CIM_Setting {

      [Key, Propagated ( "CIM_System.CreationClassName" ), 
       Description (
          "The scoping System's CreationClassName."), 
       MaxLen ( 256 )]
   string SystemCreationClassName;

      [Key, Propagated ( "CIM_System.Name" ), Description (
          "The scoping System's Name."), 
       MaxLen ( 256 )]
   string SystemName;

      [Key, Description (
          "CreationClassName indicates the name of the class or the "
          "subclass used in the creation of an instance. When used "
          "with the other key properties of this class, this property "
          "allows all instances of this class and its subclasses to be "
          "uniquely identified."), 
       MaxLen ( 256 )]
   string CreationClassName;

      [Key, Override ( "SettingID" ), MaxLen ( 256 )]
   string SettingID;
};


// ==================================================================
// SettingForSystem
// ==================================================================
   [Association, Version ( "2.8.0" ), Description (
       "CIM_SettingForSystem defines a Setting in the context of the "
       "System on which it resides.")]
class CIM_SettingForSystem : CIM_HostedDependency {

      [Override ( "Antecedent" ), Min ( 1 ), Max ( 1 ), Description (
          "The hosting System.")]
   CIM_System REF Antecedent;

      [Override ( "Dependent" ), Weak, Description (
          "The Setting defined for the System.")]
   CIM_SystemSetting REF Dependent;
};


// ===================================================================
// Configuration
// ===================================================================
   [Version ( "2.6.0" ), Description (
       "The Configuration object allows the grouping of sets of "
       "parameters (defined in Setting objects) and dependencies for "
       "one or more ManagedSystemElements. It represents a certain "
       "behavior, or a desired functional state for the ManagedSystem "
       "Elements. Note that the CIM_Profile class uses simplified "
       "naming/identity and collection algorithms as compared to "
       "CIM_Configuration. \n"
       "The desired functional state of the Configuration is typically "
       "driven by external requirements such as time or location. For "
       "example, to connect to a Mail System from 'home', a dependency "
       "on a modem exists, but a dependency on a network adapter "
       "exists at 'work'. Settings for the pertinent LogicalDevices "
       "(in this example, POTSModem and NetworkAdapter) can be defined "
       "and aggregated by the Configuration. Therefore, two 'Connect "
       "to Mail' Configurations may be defined grouping the relevant "
       "dependencies and Setting objects.")]
class CIM_Configuration : CIM_ManagedElement {

      [Key, Description (
          "The label by which the Configuration object is known."), 
       MaxLen ( 256 )]
   string Name;
};


// ===================================================================
// ConfigurationComponent
// ===================================================================
   [Association, Aggregation, Version ( "2.6.0" ), Description (
       "ConfigurationComponent aggregates 'lower-level' Configuration "
       "objects into a 'high-level' Configuration. This enables the "
       "assembly of complex Configurations by grouping together "
       "simpler ones. For example, a logon policy for the United "
       "States could consist of two Configuration groups, one for the "
       "east coast and one for the west coast. Each of these could in "
       "turn consist of multiple Configurations to handle different "
       "aspects of the logon process.")]
class CIM_ConfigurationComponent {

      [Key, Aggregate, Description (
          "The Configuration that aggregates additional "
          "Configurations.")]
   CIM_Configuration REF ConfigGroup;

      [Key, Description (
          "A Configuration that is part of a 'higher-level' "
          "Configuration.")]
   CIM_Configuration REF ConfigComponent;
};


// ===================================================================
// ElementConfiguration
// ===================================================================
   [Association, Version ( "2.6.0" ), Description (
       "This association relates a Configuration object to one or more "
       "ManagedSystemElements. The Configuration object represents a "
       "certain behavior, or a desired functional state for the "
       "associated ManagedSystemElements.")]
class CIM_ElementConfiguration {

      [Key, Description (
          "The ManagedSystemElement.")]
   CIM_ManagedSystemElement REF Element;

      [Key, Description (
          "The Configuration object that groups the Settings and "
          "dependencies associated with the ManagedSystemElement.")]
   CIM_Configuration REF Configuration;
};


// ===================================================================
// CollectionConfiguration
// ===================================================================
   [Association, Version ( "2.6.0" ), Description (
       "This association relates a Configuration object to one or more "
       "CollectionOfMSEs objects. The Configuration object represents "
       "a certain behavior, or a desired functional state for the "
       "associated Collection.")]
class CIM_CollectionConfiguration {

      [Key, Description (
          "The CollectionOfMSEs.")]
   CIM_CollectionOfMSEs REF Collection;

      [Key, Description (
          "The Configuration object that groups the Settings and "
          "dependencies associated with the Collection.")]
   CIM_Configuration REF Configuration;
};


// ===================================================================
// DependencyContext
// ===================================================================
   [Association, Aggregation, Version ( "2.6.0" ), Description (
       "This relationship associates a Dependency with one or more "
       "Configuration objects. For example, a ComputerSystem's "
       "dependencies could change based on the site/network to which "
       "the System is attached.")]
class CIM_DependencyContext {

      [Key, Aggregate, Description (
          "The Configuration object that aggregates the Dependency.")]
   CIM_Configuration REF Context;

      [Key, Description (
          "An aggregated Dependency.")]
   CIM_Dependency REF Dependency;
};


// ===================================================================
// SettingContext
// ===================================================================
   [Association, Aggregation, Version ( "2.6.0" ), Description (
       "This relationship associates Configuration objects with "
       "Setting objects. For example, a NetworkAdapter's Settings "
       "could change based on the site/network to which its hosting "
       "ComputerSystem is attached. In this case, the ComputerSystem "
       "would have two different Configuration objects, corresponding "
       "to the differences in network configuration for the two "
       "network segments. Configuration A would aggregate a Setting "
       "object for the NetworkAdapter when operating on segment "
       "\"ANet\", whereas Configuration B would aggregate a different "
       "NetworkAdapter Setting object, specific to segment \"BNet\". "
       "Note that many Settings of the computer are independent of the "
       "network Configuration. For example, both Configurations A and "
       "B would aggregate the same Setting object for the "
       "ComputerSystem's MonitorResolution.")]
class CIM_SettingContext {

      [Key, Aggregate, Description (
          "The Configuration object that aggregates the Setting.")]
   CIM_Configuration REF Context;

      [Key, Description (
          "An aggregated Setting.")]
   CIM_Setting REF Setting;
};


// ===================================================================
// CollectionSetting
// ===================================================================
   [Association, Version ( "2.6.0" ), Description (
       "CollectionSetting represents the association between a "
       "CollectionOfMSEs class and the Setting class(es) defined for "
       "them.")]
class CIM_CollectionSetting {

      [Key, Description (
          "The CollectionOfMSEs.")]
   CIM_CollectionOfMSEs REF Collection;

      [Key, Description (
          "The Setting object associated with the Collection.")]
   CIM_Setting REF Setting;
};


// ==================================================================
// SystemConfiguration
// ==================================================================
   [Version ( "2.6.0" ), Description (
       "CIM_SystemConfiguration represents the general concept of a "
       "CIM_Configuration which is scoped by/weak to a System. This "
       "class is a peer of CIM_Configuration since the key structure "
       "of Configuration is currently defined and cannot be modified "
       "with additional properties.")]
class CIM_SystemConfiguration : CIM_ManagedElement {

      [Key, Propagated ( "CIM_System.CreationClassName" ), 
       Description (
          "The scoping System's CreationClassName."), 
       MaxLen ( 256 )]
   string SystemCreationClassName;

      [Key, Propagated ( "CIM_System.Name" ), Description (
          "The scoping System's Name."), 
       MaxLen ( 256 )]
   string SystemName;

      [Key, Description (
          "CreationClassName indicates the name of the class or the "
          "subclass used in the creation of an instance. When used "
          "with the other key properties of this class, this property "
          "allows all instances of this class and its subclasses to be "
          "uniquely identified."), 
       MaxLen ( 256 )]
   string CreationClassName;

      [Key, Description (
          "The label by which the Configuration object is known."), 
       MaxLen ( 256 )]
   string Name;
};


// ==================================================================
// ConfigurationForSystem
// ==================================================================
   [Association, Version ( "2.8.0" ), Description (
       "CIM_ConfigurationForSystem defines a Configuration in the "
       "context of the System on which it resides.")]
class CIM_ConfigurationForSystem : CIM_HostedDependency {

      [Override ( "Antecedent" ), Min ( 1 ), Max ( 1 ), Description (
          "The hosting System.")]
   CIM_System REF Antecedent;

      [Override ( "Dependent" ), Weak, Description (
          "The Configuration defined for the System.")]
   CIM_SystemConfiguration REF Dependent;
};


// ==================================================================
// SystemSettingContext
// ==================================================================
   [Association, Aggregation, Version ( "2.6.0" ), Description (
       "This relationship associates System-specific Configuration "
       "objects with System-specific Setting objects, similar to the "
       "SettingContext association.")]
class CIM_SystemSettingContext {

      [Key, Aggregate, Description (
          "The Configuration object that aggregates the Setting.")]
   CIM_SystemConfiguration REF Context;

      [Key, Description (
          "An aggregated Setting.")]
   CIM_SystemSetting REF Setting;
};


// ===================================================================
// end of file
// ===================================================================
