// ===================================================================
// Title:       Device Network Adapters 2.7
// Filename:    Device27_NetworkAdapter.mof
// Version:     2.7.0
// Release:     Final
// Date:        04/02/03
// ===================================================================
// Copyright 1998-2003 Distributed Management Task Force, Inc. (DMTF).
// All rights reserved.  
// DMTF is a not-for-profit association of industry members dedicated 
// to promoting enterprise and systems management and interoperability. 
// DMTF specifications and documents may be reproduced for uses
// consistent with this purpose by members and non-members, 
// provided that correct attribution is given. 
// As DMTF specifications may be revised from time to time, 
// the particular version and release date should always be noted.
//
// Implementation of certain elements of this standard or proposed 
// standard may be subject to third party patent rights, including 
// provisional patent rights (herein "patent rights"). DMTF makes 
// no representations to users of the standard as to the existence 
// of such rights, and is not responsible to recognize, disclose, or
// identify any or all such third party patent right, owners or 
// claimants, nor for any incomplete or inaccurate identification or 
// disclosure of such rights, owners or claimants. DMTF shall have no 
// liability to any party, in any manner or circumstance, under any 
// legal theory whatsoever, for failure to recognize, disclose, or 
// identify any such third party patent rights, or for such party's
// reliance on the standard or incorporation thereof in its product, 
// protocols or testing procedures. DMTF shall have no liability to 
// any party implementing such standard, whether such implementation 
// is foreseeable or not, nor to any patent owner or claimant, and shall 
// have no liability or responsibility for costs or losses incurred if 
// a standard is withdrawn or modified after publication, and shall be
// indemnified and held harmless by any party implementing the 
// standard from any and all claims of infringement by a patent owner 
// for such implementations.
//
// For information about patents held by third-parties which have 
// notified the DMTF that, in their opinion, such patent may relate to 
// or impact implementations of DMTF standards, visit 
// http://www.dmtf.org/about/policies/disclosures.php.
// ===================================================================
// Description: The Device Model extends the management concepts that
//              are related to LogicalDevices. This file refines 
//              the original concepts related to representing 
//              network ports as adapters.
//
//              The object classes below are listed in an order that
//              avoids forward references. Required objects, defined 
//              by other working groups, are omitted.
// ==================================================================
// Change Log for v2.7
// CR630 - Deprecate the statistical properties in NetworkAdapter
//       - Deprecate FibreChannelAdapter, FCAdapterEventCounters,    
//         FibrePort, FibrePortEventCounters, FibrePortOnFCAdapter      
//         and FibrePortActiveLogin      
// CR783 - Deprecate NetworkAdapter, EthernetAdapter, 
//         TokenRingAdapter, OOBAlertServiceOnNetworkAdapter, 
//         WakeUpServiceOnNetworkAdapter, NetworkVirtualAdapter
//         and NetworkAdapterRedundancyComponent
// CR845 - Deprecate AdapterActiveConnection
//       - Change deprecation of NetworkVirtualAdapter to 
//         ConcreteIdentity
// CR860 - Add the Deprecated qualifier to the individual properties
//         of the Deprecated Fibre Channel classes
// ================================================================== 

#pragma locale ("en_US")
 
 
// ===================================================================
// NetworkAdapter 
// ===================================================================
[Abstract, Deprecated {"CIM_NetworkPort"}, Version ("2.7.0"), 
    Description (
        "The use of the CIM_NetworkAdpater class has been "
        "deprecated in lieu of CIM_NetworkPort. This better reflects "
        "that the hardware of a single port is described and managed. "
        "NetworkAdapter is an Abstract class defining general "
        "networking hardware concepts (for example, PermanentAddress "
        "or Speed of operation).") ]
class CIM_NetworkAdapter : CIM_LogicalDevice {
 
    [Deprecated {"CIM_NetworkPort.PermanentAddress"}, 
        MaxLen (64), Description (
        "PermanentAddress defines the network address hardcoded into "
        "an adapter.  This 'hardcoded' address may be changed via "
        "firmware upgrade or software configuration. If so, this field "
        "should be updated when the change is made.  PermanentAddress "
        "should be left blank if no 'hardcoded' address exists for the "
        "NetworkAdapter."),
        MappingStrings {"MIF.DMTF|Network Adapter 802 Port|001.2"} ]       
    string PermanentAddress;
 
    [Deprecated {"CIM_NetworkPort.NetworkAddress"}, 
        MaxLen (64), Description (
        "An array of strings indicating the network addresses for an "
        "adapter."),
        ArrayType ("Indexed"),
        MappingStrings {"MIF.DMTF|Network Adapter 802 Port|001.3"} ]
    string NetworkAddresses[]; 
 
    [Deprecated {"CIM_NetworkPort.Speed"}, Description (
        "An estimate of the current bandwidth in Bits per Second. "
        "For Adapters which vary in bandwidth or for those where "
        "no accurate estimation can be made, this property should "
        "contain the nominal bandwidth."),
        Units ("Bits per Second"), 
        MappingStrings {"MIB.IETF|RFC1213-MIB.ifSpeed", 
            "MIF.DMTF|Network Adapter 802 Port|001.5"} ]
    uint64 Speed;
 
    [Deprecated {"CIM_NetworkPort.MaxSpeed"}, Description ( 
        "The maximum speed, in Bits per Second, for the Network"
        "Adapter."), 
        Units ("Bits per Second")  ] 
    uint64 MaxSpeed;
 
    [Deprecated {"CIM_NetworkPort.FullDuplex"}, Description (
        "Boolean indicating that the Adapter is operating in "
        "full duplex mode.") ]
    boolean FullDuplex;
 
    [Deprecated {"CIM_NetworkPort.AutoSense"}, Description ( 
        "A boolean indicating whether the NetworkAdapter is capable " 
        "of automatically determining the speed or other "
        "communications characteristics of the attached network "
        "media.")  ] 
    boolean AutoSense;
 
    [Deprecated {"CIM_NetworkPortStatistics.BytesTransmitted"}, 
        Description (
        "The use of OctetsTransmitted is deprecated.  The replacement "
        "is CIM_NetworkPortStatistics.BytesTransmitted."),
        Mappingstrings {"MIB.IETF|RFC1213-MIB.ifOutOctets", 
            "MIF.DMTF|Network Adapter 802 Port|001.7"}, 
        Counter ] 
    uint64 OctetsTransmitted;
    
    [Deprecated {"CIM_NetworkPortStatistics.BytesReceived"}, 
        Description (
        "The use of OctetsReceived is deprecated.  The replacement is "
        "CIM_NetworkPortStatistics.BytesReceived."),
        Mappingstrings {"MIB.IETF|RFC1213-MIB.ifInOctets",
            "MIF.DMTF|Network Adapter 802 Port|001.9"}, 
        Counter ] 
    uint64 OctetsReceived;
};


// ===================================================================
// EthernetAdapter
// ===================================================================
[Deprecated {"CIM_ EthernetAdapter"}, Version ("2.7.0"), 
    Description (
        "The use of the CIM_EthernetAdapter class has been deprecated, "
        "consistent with NetworkAdapter. Instead use the CIM_"
        "EthernetPort class. This class describes the capabilities "
        "and management aspects of an EthernetAdapter.") ]
class CIM_EthernetAdapter : CIM_NetworkAdapter {
 
    [Deprecated {"CIM_EthernetPort.NetworkAddresses"}, 
        Override ("NetworkAddresses"), 
        Description (
        "Ethernet/802.3 MAC addresses formatted as twelve hexadecimal "
        "digits (e.g. \"010203040506\"), with each pair representing "
        "one of the six octets of the MAC address in \"canonical\" "
        "bit order.  (Thus, the Group address bit is found in the low "
        "order bit of the first character of the string.)"),
        ArrayType ("Indexed") ]
    string NetworkAddresses[];
 
    [Deprecated {"CIM_EthernetPortStatistics.MaxDataSize"}, 
        Description (
        "The maximum size of the INFO (non-MAC) field that will be "
        "received or transmitted."), 
        Mappingstrings {"MIB.IETF|BRIDGE-MIB.dot1dTpPortMaxInfo"} ]
    uint32 MaxDataSize;
 
    [Deprecated {"CIM_EthernetPort.Capabilities"}, 
        Description (
        "Capabilities of the EthernetAdapter. For example, the "
        "Device may support AlertOnLan, WakeOnLan, Load Balancing "
        "and/or FailOver. If failover or load balancing "
        "capabilities are listed, a SpareGroup (failover) or "
        "ExtraCapacityGroup (load balancing) should also be defined "
        "to completely describe the capability."), 
        ArrayType ("Indexed"), 
        ValueMap {"0", "1", "2", "3", "4", "5"},
        Values {"Unknown", "Other", "AlertOnLan", "WakeOnLan", 
            "FailOver", "LoadBalancing"}, 
        ModelCorrespondence {
            "CIM_EthernetAdapter.CapabilityDescriptions"} ]
    uint16 Capabilities[];
 
    [Deprecated {"CIM_EthernetPort.CapabilityDescriptions"}, 
        Description (
        "An array of free-form strings providing more detailed "
        "explanations for any of the EthernetAdapter features "
        "indicated in the Capabilities array. Note, each entry of "
        "this array is related to the entry in the Capabilities "
        "array that is located at the same index."), 
        ArrayType ("Indexed"), 
        ModelCorrespondence {"CIM_EthernetAdapter.Capabilities"} ]
    string CapabilityDescriptions[];
 
    [Deprecated {"CIM_EthernetPort.EnabledCapabilities"}, 
        Description (
        "Specifies which capabilities are enabled from the list "
        "of all supported ones, defined in the Capabilities array."), 
        ValueMap {"0", "1", "2", "3", "4", "5"},
        Values {"Unknown", "Other", "AlertOnLan", "WakeOnLan", 
            "FailOver", "LoadBalancing"}, 
        ModelCorrespondence {"CIM_EthernetAdapter.Capabilities"} ]
    uint16 EnabledCapabilities[];
 
    [Deprecated {"CIM_EthernetPortStatistics.SymbolErrors"}, 
        Description (
        "The number of times there was an invalid data symbol when "
        "a valid carrier was present. The count is incremented at "
        "most once per carrier event, even if multiple symbol "
        "errors occur during the carrier event."), 
        MappingStrings {"MIB.IETF|EtherLike-MIB.dot3StatsSymbolErrors"}, 
        Counter ] 
    uint32 SymbolErrors;
 
    [Deprecated {"CIM_NetworkPortStatistics.TotalPacketsTransmitted"}, 
        Description ("The total number of packets transmitted."), 
        MappingStrings {"MIF.DMTF|Network Adapter 802 Port|001.6"}, 
        Counter ] 
    uint64 TotalPacketsTransmitted;
 
    [Deprecated {"CIM_NetworkPortStatistics.TotalPacketsReceived"}, 
        Description ("The total number of packets received."), 
        MappingStrings {"MIF.DMTF|Network Adapter 802 Port|001.8"}, 
        Counter ] 
    uint64 TotalPacketsReceived;
 
    [Deprecated {"CIM_EthernetPortStatistics.AlignmentErrors"}, 
        Description (
        "A count of frames received on a particular interface "
        "that are not an integral number of octets in length and do "
        "not pass the FCS check. The count represented by an "
        "instance of this object is incremented when the alignment"
        "Error status is returned by the MAC layer to the LLC (or "
        "other MAC user). Received frames for which multiple error "
        "conditions obtain are, according to the conventions of IEEE "
        "802.3 Layer Management, counted exclusively according to "
        "the error status presented to the LLC."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsAlignmentErrors"}, 
        Counter ] 
    uint32 AlignmentErrors;
 
    [Deprecated {"CIM_EthernetPortStatistics.FCSErrors"}, 
        Description (
        "A count of frames received on a particular interface "
        "that are an integral number of octets in length but do "
        "not pass the FCS check. The count represented by an "
        "instance of this object is incremented when the frame"
        "CheckError status is returned by the MAC layer to the "
        "LLC (or other MAC user). Received frames for which "
        "multiple error conditions obtain are, according to the "
        "conventions of IEEE 802.3 Layer Management, counted "
        "exclusively according to the error status presented to "
        "the LLC."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsFCSErrors"}, 
        Counter ] 
    uint32 FCSErrors;
 
    [Deprecated {"CIM_EthernetPortStatistics.SingleCollisionFrames"}, 
        Description (
        "A count of successfully transmitted frames on a particular "
        "interface for which transmission is inhibited by exactly "
        "one collision. A frame that is counted by an instance of "
        "this object is not counted by the corresponding instance "
        "of the MultipleCollisionFrames property."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsSingleCollisionFrames"}, 
        Counter ] 
    uint32 SingleCollisionFrames;
 
    [Deprecated {"CIM_EthernetPortStatistics.MultipleCollisionFrames"}, 
        Description (
        "A count of successfully transmitted frames on a particular "
        "interface for which transmission is inhibited by more than "
        "one collision. A frame that is counted by an instance of "
        "this object is not counted by the corresponding instance "
        "of the SingleCollisionFrames property."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsMultipleCollisionFrames"}, 
        Counter ] 
    uint32 MultipleCollisionFrames;
 
    [Deprecated {"CIM_EthernetPortStatistics.SQETestErrors"}, 
        Description (
        "A count of times that the SQE TEST ERROR message is "
        "generated by the PLS sublayer for a particular interface. "
        "The SQE TEST ERROR message is defined in section "
        "7.2.2.2.4 of ANSI/IEEE 802.3-1985 and its generation is "
        "described in section 7.2.4.6 of the same document."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsSQETestErrors"}, 
        Counter ] 
    uint32 SQETestErrors;
 
    [Deprecated {"CIM_EthernetPortStatistics.DeferredTransmissions"}, 
        Description (
        "A count of frames for which the first transmission "
        "attempt on a particular interface is delayed because the "
        "medium is busy. The count represented by an instance of "
        "this object does not include frames involved in collisions."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsDeferredTransmissions"}, 
        Counter ] 
    uint32 DeferredTransmissions;
 
    [Deprecated {"CIM_EthernetPortStatistics.LateCollisions"}, 
        Description (
        "The number of times that a collision is detected on a "
        "particular interface later than 512 bit-times into the "
        "transmission of a packet. Five hundred and twelve bit-"
        "times corresponds to 51.2 microseconds on a 10 Mbit/s "
        "system. A (late) collision included in a count "
        "represented by an instance of this object is also "
        "considered as a (generic) collision for purposes of "
        "other collision-related statistics."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsLateCollisions"}, 
        Counter ] 
    uint32 LateCollisions;
 
    [Deprecated {"CIM_EthernetPortStatistics.ExcessiveCollisions"}, 
        Description (
        "A count of frames for which transmission on a particular "
        "interface fails due to excessive collisions."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsExcessiveCollisions"}, 
        Counter ] 
    uint32 ExcessiveCollisions;
 
    [Deprecated {"CIM_EthernetPortStatistics."
            "InternalMACTransmitErrors"}, 
        Description (
        "A count of frames for which transmission on a particular "
        "interface fails due to an internal MAC sublayer transmit "
        "error. A frame is only counted by an instance of this "
        "object if it is not counted by the corresponding instance "
        "of either the LateCollisions property, the Excessive"
        "Collisions property, or the CarrierSenseErrors property. "
        "The precise meaning of the count represented by an instance "
        "of this object is implementation-specific.  In particular, "
        "an instance of this object may represent a count of "
        "transmission errors on a particular interface that are "
        "not otherwise counted."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB."
            "dot3StatsInternalMacTransmitErrors"}, 
        Counter ] 
    uint32 InternalMACTransmitErrors;
 
    [Deprecated {"CIM_EthernetPortStatistics."
            "InternalMACReceiveErrors"}, 
        Description (
        "A count of frames for which reception on a particular "
        "interface fails due to an internal MAC sublayer receive "
        "error. A frame is only counted by an instance of this "
        "object if it is not counted by the corresponding instance "
        "of either the FrameTooLongs property, the AlignmentErrors "
        "property, or the FCSErrors property. The precise meaning "
        "of the count represented by an instance of this object is "
        "implementation-specific.  In particular, an instance of "
        "this object may represent a count of receive errors on a "
        "particular interface that are not otherwise counted."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsInternalMacReceiveErrors"}, 
        Counter ] 
    uint32 InternalMACReceiveErrors;
 
    [Deprecated {"CIM_EthernetPortStatistics.CarrierSenseErrors"}, 
        Description (
        "The number of times that the carrier sense condition was "
        "lost or never asserted when attempting to transmit a frame "
        "on a particular interface. The count represented by an "
        "instance of this object is incremented at most once per "
        "transmission attempt, even if the carrier sense condition "
        "fluctuates during a transmission attempt."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsCarrierSenseErrors"}, 
        Counter ] 
    uint32 CarrierSenseErrors;
 
    [Deprecated {"CIM_EthernetPortStatistics.FrameTooLongs"}, 
        Description (
        "A count of frames received on a particular interface that "
        "exceed the maximum permitted frame size. The count "
        "represented by an instance of this object is incremented "
        "when the FrameTooLong status is returned by the MAC layer "
        "to the LLC (or other MAC user). Received frames for which "
        "multiple error conditions obtain are, according to the "
        "conventions of IEEE 802.3 Layer Management, counted "
        "exclusively according to the error status presented to "
        "the LLC."),
        Mappingstrings {
            "MIB.IETF|EtherLike-MIB.dot3StatsFrameTooLongs"}, 
        Counter ] 
    uint32 FrameTooLongs;
};


// ===================================================================
// TokenRingAdapter
// ===================================================================
[Deprecated {"CIM_TokenRingAdapter"}, Version ("2.7.0"), 
    Description (
        "The use of the CIM_TokenRingAdapter class has been "
        "deprecated, consistent with NetworkAdapter. Instead use "
        "the CIM_TokenRingPort class. This class describes the "
        "capabilities and management aspects of a TokenRingAdapter.") ]
class CIM_TokenRingAdapter : CIM_NetworkAdapter {
 
    [Deprecated {"CIM_TokenRingAdapter.NetworkAddresses"}, 
        Override ("NetworkAddresses"), Description (
        "Token Ring/802.5 MAC addresses formatted as twelve "
        "hexadecimal digits (e.g. \"010203040506\"), with each pair "
        "representing one of the six octets of the MAC address in "
        "\"canonical\" bit order.  (Thus, the Group address bit is "
        "found in the low order bit of the first character of the "
        "string.)"),
        ArrayType ("Indexed") ]
    string NetworkAddresses[];
 
    [Deprecated {"CIM_TokenRingPort.MaxDataSize"}, 
        Description (
        "The maximum size of the INFO (non-MAC) field that will be "
        "received or transmitted."), 
        Mappingstrings {"MIB.IETF|BRIDGE-MIB.dot1dTpPortMaxInfo"} ]
    uint32 MaxDataSize;
 
    [Deprecated {"CIM_TokenRingPort.Capabilities"}, 
        Description (
        "Capabilities of the TokenRingAdapter. For example, the Device "
        "may support AlertOnLan, WakeOnLan, Load Balancing and/or "
        "Failover. If failover or load balancing capabilities are "
        "listed, a SpareGroup (failover) or ExtraCapacityGroup (load "
        "balancing) should also be defined to completely describe the "
        "capability."), 
        ArrayType ("Indexed"), 
        ValueMap {"0", "1", "2", "3", "4", "5"},
        Values {"Unknown", "Other", "AlertOnLan", "WakeOnLan", 
            "FailOver", "LoadBalancing"}, 
        ModelCorrespondence {
            "CIM_TokenRingPort.CapabilityDescriptions"} ]
    uint16 Capabilities[];
 
    [Deprecated {"CIM_TokenRingPort.CapabilityDescriptions"}, 
        Description (
        "An array of free-form strings providing more detailed "
        "explanations for any of the TokenRingAdapter features "
        "indicated in the Capabilities array. Note, each entry of "
        "this array is related to the entry in the Capabilities array "
        "that is located at the same index."), 
        ArrayType ("Indexed"), 
        ModelCorrespondence {"CIM_TokenRingAdapter.Capabilities"} ]
    string CapabilityDescriptions[];
 
    [Deprecated {"CIM_TokenRingPort.EnabledCapabilities"}, 
        Description (
        "Specifies which of the capabilities from the \"Capabilities\" "
        "property are currently enabled."), 
        ValueMap {"0", "1", "2", "3", "4", "5"},
        Values {"Unknown", "Other", "AlertOnLan", "WakeOnLan", 
            "FailOver", "LoadBalancing"}, 
        ModelCorrespondence {"CIM_TokenRingAdapter.Capabilities"} ]
    uint16 EnabledCapabilities[];
 
    [Deprecated {"CIM_TokenRingPort.RingStatus"}, 
        Description (
        "The current status which can be used to diagnose fluctuating "
        "problems that can occur on token rings, after a station has "
        "successfully been added to the ring. Before an open is "
        "completed, this object contains the value indicating "
        "\"no status\" (131072). (The RingState and RingOpenStatus "
        "properties are also provided for debugging problems when the "
        "station can not even enter the ring.) The property's value is "
        "a sum of values, one for each currently applicable condition. "
        "The following values are defined for various conditions:\n"
        "0= No Problems Detected, 32= Ring Recovery, "
        "64= Single Station, 256= Remove Received, 512= Reserved, "
        "1024= Auto-Removal Error, 2048= Lobe Wire Fault, "
        "4096= Transmit Beacon, 8192= Soft Error, 16384= Hard Error, "
        "32768= Signal Loss, 131072= No Status, Open Not Completed."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingStatus"} ]
    uint32 RingStatus;
 
    [Deprecated {"CIM_TokenRingPort.RingState"}, 
        Description (
        "The current Device state with respect to entering or leaving "
        "the ring."), 
        ValueMap {"0", "1", "2", "3", "4", "5"},
        Values {"Opened", "Closed", "Opening", "Closing", 
            "Open Failure", "Ring Failure"}, 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingState"} ]
    uint16 RingState;
 
    [Deprecated {"CIM_TokenRingPort.RingOpenStatus"}, 
        Description (
        "This property indicates the success, or the reason for "
        "failure, of the station's most recent attempt to enter "
        "the ring."), 
        ValueMap {"0", "1", "2", "3", "4", "5", "6", "7", "8", "9", 
            "10"},
        Values {"No Open Attempted", "Bad Parameter", "Lobe Failed", 
            "Signal Loss", "Insertion Timeout", "Ring Failed", 
            "Beaconing", "Duplicate MAC", "Request Failed", 
            "Remove Received", 
            // 10
            "Last Open Successful"}, 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingOpenStatus"} ]
    uint16 RingOpenStatus;
 
    [Deprecated {"CIM_TokenRingPort.RingSpeed"}, 
        Description ("The ring's bandwidth."), 
        ValueMap {"0", "1", "2", "3", "4"},
        Values {"Unknown", "Other", "One Megabit", "Four Megabit", 
            "Sixteen Megabit"}, 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingSpeed"} ]
    uint16 RingSpeed;
 
    [Deprecated {"CIM_TokenRingPortStatistics.BurstErrors"}, 
        Description (
        "This counter is incremented when a station detects the "
        "absence of transitions for five half-bit timers (burst-five "
        "errors)."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsBurstErrors"},
        Counter ] 
    uint32 BurstErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.ACErrors"}, 
        Description (
        "This counter is incremented when a station receives an AMP "
        "or SMP frame in which A is equal to C is equal to 0, and then "
        "receives another SMP frame with A equal to C equal to 0 "
        "without first receiving an AMP frame. It denotes a station "
        "that cannot set the AC bits properly."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsACErrors"}, 
        Counter ] 
    uint32 ACErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.AbortTransErrors"}, 
        Description (
        "This counter is incremented when a station transmits an abort "
        "delimiter while transmitting data."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB."
            "dot5StatsAbortTransErrors"}, 
        Counter ] 
    uint32 AbortTransErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.InternalErrors"}, 
        Description (
        "This counter is incremented when a station recognizes an "
        "internal error."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB."
            "dot5StatsInternalErrors"}, 
        Counter ] 
    uint32 InternalErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.LostFrameErrors"}, 
        Description (
        "This counter is incremented when a station is transmitting "
        "and its TRR timer expires. This denotes a condition where a "
        "transmitting station in strip mode does not receive the "
        "trailer of the frame before the TRR timer goes off."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB."
            "dot5StatsLostFrameErrors"},
        Counter ] 
    uint32 LostFrameErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.ReceiveCongestions"}, 
        Description (
        "This counter is incremented when a station recognizes a frame "
        "addressed to its specific address, but has no available "
        "buffer space - indicating that the station is congested."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB."
            "dot5StatsReceiveCongestions"}, 
        Counter ] 
    uint32 ReceiveCongestions;
 
    [Deprecated {"CIM_TokenRingPortStatistics.FrameCopiedErrors"}, 
        Description (
        "This counter is incremented when a station recognizes a frame "
        "addressed to its specific address and detects that the FS "
        "field A bits are set to 1 indicating a possible line hit or "
        "duplicate address."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB."
            "dot5StatsFrameCopiedErrors"}, 
        Counter ] 
    uint32 FrameCopiedErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.TokenErrors"}, 
        Description (
        "This counter is incremented when a station acting as the "
        "active monitor recognizes an error condition that needs a "
        "token transmitted."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsTokenErrors"},
        Counter ]
    uint32 TokenErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.SoftErrors"}, 
        Description (
        "The number of Soft Errors that the Device has detected. It "
        "directly corresponds to the number of Report Error MAC frames "
        "that this Device has transmitted. Soft Errors are those which "
        "are recoverable by the MAC layer protocols."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsSoftErrors"}, 
        Counter ]
    uint32 SoftErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.HardErrors"}, 
        Description (
        "The number of times this Device has detected an immediately "
        "recoverable fatal error. It denotes the number of times this "
        "Device is either transmitting or receiving beacon MAC "
        "frames."),
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsHardErrors"}, 
        Counter ]
    uint32 HardErrors;
 
    [Deprecated {"CIM_TokenRingPortStatistics.SignalLossCount"}, 
        Description (
        "The number of times this Device has detected the loss of "
        "signal condition from the ring."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsSignalLoss"},
        Counter ]
    uint32 SignalLossCount;
 
    [Deprecated {"CIM_TokenRingPortStatistics.TransmittedBeacons"}, 
        Description (
        "The number of times this Device has transmitted a beacon "
        "frame."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB."
            "dot5StatsTransmitBeacons"}, 
        Counter ]
    uint32 TransmittedBeacons;
 
    [Deprecated {"CIM_TokenRingPortStatistics.Recoverys"}, 
        Description (
        "The number of Claim Token MAC frames received or transmitted "
        "after the Device has received a Ring Purge MAC frame. This "
        "counter signifies the number of times the ring has been "
        "purged and is being recovered back into a normal operating "
        "state."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsRecoverys"}, 
        Counter ]
    uint32 Recoverys;
 
    [Deprecated {"CIM_TokenRingPortStatistics.LobeWires"}, 
        Description (
        "The number of times the Device has detected an open or short "
        "circuit in the lobe data path. The adapter will be closed and "
        "RingState will signify this condition."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsLobeWires"}, 
        Counter ]
    uint32 LobeWires;
 
    [Deprecated {"CIM_TokenRingPortStatistics.Removes"}, 
        Description (
        "The number of times the Device has received a Remove Ring "
        "Station MAC frame request. When this frame is received, the "
        "Device will enter the close state and RingState will "
        "signify this condition."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsRemoves"}, 
        Counter ]
    uint32 Removes;
 
    [Deprecated {"CIM_TokenRingPortStatistics.Singles"}, 
        Description (
        "The number of times the Device has sensed that it is the "
        "only station on the ring. This will happen if the Device "
        "is the first one up on a ring, or if there is a hardware "
        "problem."), 
        MappingStrings {
            "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsSingles"}, 
        Counter ]
    uint32 Singles;
 
    [Deprecated {"CIM_TokenRingPortStatistics.FrequencyErrors"}, 
        Description (
        "The number of times the Device has detected that the "
        "frequency of the incoming signal differs from the expected "
        "frequency by more than that specified by the IEEE 802.5 "
        "standard."), 
        MappingStrings {
           "MIB.IETF|IEEE 802.5 Token Ring MIB.dot5StatsFreqErrors"}, 
        Counter ]
    uint32 FrequencyErrors;
};


// ===================================================================
// OOBAlertServiceOnNetworkAdapter 
// ===================================================================
[Association, Deprecated {"CIM_OOBAlertServiceOnNetworkPort"}, 
    Version ("2.7.0"), Description (
        "The use of the CIM_OOBAlertServiceOnNetworkAdapter class "
        "has been deprecated, since NetworkAdapter has been deprecated. "
        "Instead use the CIM_OOBAlertServiceOnNetworkPort class. "
        "OOBAlertServiceOnNetworkAdapter defines where the "
        "out of band alerting Service is implemented.") ]
class CIM_OOBAlertServiceOnNetworkAdapter : 
 CIM_DeviceServiceImplementation {
 
    [Override ("Antecedent"), Max (1), Deprecated {
        "CIM_OOBAlertServiceOnNetworkPort.Antecedant"}, 
        Description (
            "The NetworkAdapter which implements the Service.") ]
    CIM_NetworkAdapter REF Antecedent;
 
    [Override ("Dependent"), Deprecated {
        "CIM_OOBAlertServiceOnNetworkPort.Dependent"}, 
        Description (
            "The alerting Service provided on the NetworkAdapter.") ]
    CIM_OOBAlertService REF Dependent;
};
 
 
// ===================================================================
// WakeUpServiceOnNetworkAdapter 
// ===================================================================
[Association, Deprecated {"CIM_WakeUpServiceOnNetworkPort"}, 
    Version ("2.7.0"), Description (
        "The use of the CIM_WakeUpServiceOnNetworkAdapter class has "
        "been deprecated, since NetworkAdapter is deprecated. Instead "
        "use the CIM_WakeUpServiceOnNetworkPort class. "
        "WakeUpServiceOnNetworkAdapter defines where the "
        "WakeUpService is implemented.") ]
class CIM_WakeUpServiceOnNetworkAdapter : 
 CIM_DeviceServiceImplementation {
 
    [Override ("Antecedent"), Max (1), Deprecated {
        "CIM_WakeUpServiceOnNetworkPort.Antecedent"}, 
        Description (
            "The NetworkAdapter which implements the Service.") ]
    CIM_NetworkAdapter REF Antecedent;
 
    [Override ("Dependent"), 
        Deprecated {"CIM_WakeUpServiceOnNetworkPort.Dependent"}, 
        Description (
            "The wakeup Service provided on the NetworkAdapter.") ]
    CIM_WakeUpService REF Dependent;
};
 
 
// ===================================================================
// NetworkAdapterRedundancyComponent
// ===================================================================
[Association, Deprecated {"CIM_OrderedMemberOfCollection"}, 
    Version ("2.7.0"), Description (
        "The use of the CIM_NetworkAdapterRedundancyComponent class "
        "has been deprecated since a specific association is not "
        "needed. Instead use the CIM_ OrderedMemberOf"
        "Collection class. CIM_NetworkAdapterRedundancyComponent "
        "indicates the role that a NetworkAdapter plays in a "
        "ExtraCapacityGroup, providing load balancing.") ]
class CIM_NetworkAdapterRedundancyComponent : CIM_RedundancyComponent {
 
    [Override("GroupComponent"), Aggregate,
        Deprecated {"CIM_OrderedMemberOfCollection.Collection"}, 
        Description (
            "The RedundancyGroup representing a set of load balanced "
            "NetworkAdapters.") ]
    CIM_ExtraCapacityGroup REF GroupComponent;
 
    [Override("PartComponent"), 
        Deprecated {"CIM_OrderedMemberOfCollection.Member"}, 
        Description (
            "The Network Adapter(s) belonging to the "
            "RedundancyGroup.") ]
    CIM_NetworkAdapter REF PartComponent;
 
    [Deprecated {"No value"}, Description (
        "Indicates the scope of load balancing for the NetworkAdapters "
        "involved in the RedundancyGroup. Load balancing may be "
        "restricted to transmitting data only (value=1), "
        "receiving data only (value=2), or used for both transmit "
        "and receive (value=3)."), 
        ValueMap {"0", "1", "2", "3"},
        Values {"Unknown", "Load Balancing - Transmit Only",
            "Load Balancing - Receive Only", "Full Load Balancing"} ]
    uint16 ScopeOfBalancing;
 
    [Deprecated {"CIM_OrderedMemberOfCollection.AssignedSequence"}, 
        Description (
            "Boolean indicating whether the Network Adapter is an "
            "original primary adapter (value=1), a preferred primary "
            "adapter (2), or both (3). Values of \"Unknown\" and "
            "\"Not Applicable\" may also be specified."),
        ValueMap {"0", "1", "2", "3", "4"},
        Values {"Unknown", "Original Primary", "Preferred Primary", 
            "Both", "Not Applicable"} ]
    uint16 PrimaryAdapter;
};
 
 
// ===================================================================
// NetworkVirtualAdapter
// ===================================================================
[Association, Deprecated {"CIM_ConcreteIdentity"}, Version ("2.7.0"),
    Description (
        "The use of the CIM_NetworkVirtualAdapter class has been "
        "deprecated. A specific association is not needed. Instead "
        "use the CIM_ConcreteIdentity class. NetworkVirtual"
        "Adapter describes that an instance of NetworkAdapter "
        "is actually the result of several Adapters "
        "participating in a load balanced RedundancyGroup.") ]
class CIM_NetworkVirtualAdapter : CIM_LogicalIdentity {
    
    [Override ("SystemElement"), 
        Deprecated {"CIM_ConcreteIdentity.SystemElement"}, 
        Description ("The 'virtual' NetworkAdapter.") ]
    CIM_NetworkAdapter REF SystemElement;
    
    [Override ("SameElement"), 
        Deprecated {"CIM_ConcreteIdentity.SameElement"}, 
        Description (
            "The ExtraCapacity RedundancyGroup that describes the "
            "load balancing. The result of the load balancing is "
            "the 'virtual' Adapter.")  ]
    CIM_ExtraCapacityGroup REF SameElement;
};
 

// ===================================================================
// AdapterActiveConnection 
// ===================================================================
[Association, Deprecated {"CIM_PortActiveConnection"}, 
    Version ("2.7.0"), Description (
        "The use of the CIM_AdapterActiveConnection class has been "
        "deprecated, since NetworkAdapter is deprecated. Instead "
        "use the CIM_PortActiveConnection class. The "
        "AdapterActiveConnection relationship indicates that a "
        "NetworkAdapter is using the referenced PhysicalConnector "
        "to output to the network. This relationship is important when "
        "the Adapter can choose to output from one of several "
        "Connectors. The Connectors may be associated with the "
        "NetworkAdapter in a Realizes relationship - but this is not "
        "required. This association provides additional information "
        "(i.e., 'in use for communication') different than Realizes.") ]
class CIM_AdapterActiveConnection : CIM_Dependency {
    
    [Override ("Antecedent"), 
        Deprecated {"CIM_PortActiveConnection.Antecedent"},  
        Description (
            "The PhysicalConnector.") ]
    CIM_PhysicalConnector REF Antecedent;
    
    [Override ("Dependent"), 
        Deprecated {"CIM_PortActiveConnection.Dependent"},   
        Description (
            "The NetworkAdapter that transmits using the "
            "Connector.") ]
    CIM_NetworkAdapter REF Dependent;
};

 
// ==================================================================
// FibreChannelAdapter 
// ==================================================================
[Version ("2.7.0"), Deprecated {"CIM_FCPort"}, Description (
    "The use of the CIM_FibreChannelAdapter class is deprecated, "
    "consistent with the deprecation of NetworkAdapter. Instead "
    "use CIM_FCPort. This class describes the capabilities "
    "and management aspects of a Fibre Channel Adapter.") ]
class CIM_FibreChannelAdapter : CIM_NetworkAdapter {

   [Deprecated {"CIM_NetworkPort.SupportedMaximumTransmissionUnit"}, 
       Description (
           "The maximum frame size, in bytes, supported by the Adapter."), 
       Units ("Bytes") ]
   uint64 MaxFrameSize;

   [Deprecated {"CIM_FCPort.SupportedCOS"}, Description (
       "The Fibre Channel Classes of Service that are supported by "
       "the Adapter, on its Ports. The currently negotiated COS for a "
       "connection is a property (NegotiatedCOS) on the FibrePort"
       "ActiveLogin association."), 
       ValueMap {"0", "1", "2", "3", "4", "5", "6"},  
       Values {"Unknown", "1", "2", "3", "4", "6", "F"} ]
   uint16 SupportedCOS[];

   [Deprecated {"CIM_FCPort.SupportedFC4Types"}, Description (
       "An array of integers indicating the Fibre Channel FC-4 "
       "protocols supported by the Adapter. The protocols that are "
       "active and running are indicated in the CurrentFC4Types "
       "property. The values used in this array are taken from the "
       "FC-GS2 (bitmapped) field defined in Table 11 of the standard. "
       "Also, FC-SB-2 codes are included from the T11 document, "
       "236V0. If the FC4 Type is \"Vendor Unique\" (value=255), "
       "then the specific vendor values (in the range, 0xE0 to 0xFF) "
       "should be listed in the FC4VendorUniqueTypes property."), 
       ValueMap {"0", "1", "4", "5", "8", "9", "17", "18", "19", "21", 
           "22", "23", "25", "26", "27", "28", "32", "34", "36", 
           "64", "80", "81", "82", "88", "96", "255"}, 
       Values {"Unknown", "Other", "ISO/IEC 8802 - 2 LLC", 
           "IP over FC", "SCSI - FCP", "SCSI - GPP", 
           "IPI - 3 Master", "IPI - 3 Slave", "IPI - 3 Peer", 
           "CP IPI - 3 Master", "CP IPI - 3 Slave", 
           "CP IPI - 3 Peer", "SBCCS Channel", 
           "SBCCS Control Unit", "FC-SB-2 Channel", 
           "FC-SB-2 Control Unit", 
           "Fibre Channel Services (FC-GS, FC-GS-2, FC-GS-3)", 
           "FC-SW", "FC - SNMP", "HIPPI - FP", "BBL Control", 
           "BBL FDDI Encapsulated LAN PDU", 
           "BBL 802.3 Encapsulated LAN PDU", "FC - VI", "FC - AV", 
           "Vendor Unique"}, 
       ModelCorrespondence {
           "CIM_FibreChannelAdapter.FC4VendorUniqueTypes"} ]
   uint16 FC4TypesSupported[];

   [MinValue (240), MaxValue (255), 
       Deprecated {"CIM_FCPort.SupportedFC4Types"}, 
       Description (
           "When the FC4TypesSupported array contains the value 255 "
           "(\"Vendor Unique\"), then the property, FC4Vendor"
           "UniqueTypes, lists of all the vendor specific protocols "
           "supported by the Adapter. These values are in the range, "
           "0xE0 to 0xFF.") ]
   uint16 FC4VendorUniqueTypes[];

   [Deprecated {"CIM_FCPort.ActiveFC4Type"}, Description (
       "An array of integers indicating the Fibre Channel FC-4 "
       "protocols currently running on the Adapter. A list of all "
       "protocols supported by the Adapter is indicated in the "
       "FC4TypesSupported property. The values used in this array "
       "are taken from the FC-GS2 (bitmapped) field defined in "
       "Table 11 of the standard. Also, FC-SB-2 codes are included "
       "from the T11 document, 236V0. If the FC4 Type is \"Vendor "
       "Unique\" (value=255), then the specific vendor values "
       "(in the range, 0xE0 to 0xFF) that are currently running "
       "should be listed in the CurrentFC4VendorTypes property."), 
       ValueMap {"0", "1", "4", "5", "8", "9", "17", "18", "19", "21", 
           "22", "23", "25", "26", "27", "28", "32", "34", "36", 
           "64", "80", "81", "82", "88", "96", "255"}, 
       Values {"Unknown", "Other", "ISO/IEC 8802 - 2 LLC", 
           "IP over FC", "SCSI - FCP", "SCSI - GPP", 
           "IPI - 3 Master", "IPI - 3 Slave", "IPI - 3 Peer", 
           "CP IPI - 3 Master", "CP IPI - 3 Slave", 
           "CP IPI - 3 Peer", "SBCCS Channel", 
           "SBCCS Control Unit", "FC-SB-2 Channel", 
           "FC-SB-2 Control Unit", 
           "Fibre Channel Services (FC-GS, FC-GS-2, FC-GS-3)", 
           "FC-SW", "FC - SNMP", "HIPPI - FP", "BBL Control", 
           "BBL FDDI Encapsulated LAN PDU", 
           "BBL 802.3 Encapsulated LAN PDU", "FC - VI", "FC - AV", 
           "Vendor Unique"}, 
       ModelCorrespondence {
           "CIM_FibreChannelAdapter.FC4TypesSupported", 
           "CIM_FibreChannelAdapter.CurrentFC4VendorTypes"} ]
   uint16 CurrentFC4Types[];

   [MinValue (240), MaxValue (255), 
       Deprecated {"CIM_FCPort.ActiveFC4Type"}, Description (
           "When the CurrentFC4Types array contains the value 255 "
           "(\"Vendor Unique\"), then the property, CurrentFC4"
           "VendorTypes, lists all the vendor specific protocols "
           "running on the Adapter. These values are in the range, "
           "0xE0 to 0xFF."), 
       ModelCorrespondence {
           "CIM_FibreChannelAdapter.FC4VendorUniqueTypes"} ]
   uint16 CurrentFC4VendorTypes[];

   [Deprecated {"No value"}, Description (
       "A list of the Capabilities of the Fibre Channel Adapter. "
       "For example, that the Adapter utilizes the Directory Server, "
       "or that it generates State Change Notifications can be "
       "indicated using the values 2 and 12, respectively."), 
       ArrayType ("Indexed"), 
       ValueMap {"0", "1", "2", "3", "4", "5", "6", "7", "8", "9", 
            "10", "11", "12", "13", "14", "15"},  
       Values {"Unknown", "Other", "Utilizes the Directory Server", 
            "Utilizes the Time Server", 
            "Utilizes the Management Server", 
            "Utilizes the Alias Server", 
            "Utilizes the Security Key Distribution Server", 
            "Utilizes the Clock Synchronization Server", 
            "Utilizes the Multicast Server", 
            "Utilizes QoS Facilitator", 
            "Utilizes Broadcast Services", 
            "Supports Fabric Login Server", 
            "Generates State Change Notifications", 
            "Registers for State Change Notifications", 
            "Responds to Read Connection Status", 
            "Supports Third Party Process Logout"} ]
   uint16 Capabilities[];

   [Deprecated {"No value"}, Description (
       "An array of free-form strings providing more detailed "
       "explanations for any of the Adapter features indicated in "
       "the Capabilities array. Note, each entry of this array "
       "is related to the entry in the Capabilities array that "
       "is located at the same index."),
       ArrayType ("Indexed"),
       ModelCorrespondence {"CIM_FibreChannelAdapter.Capabilities"} ]
   string CapabilityDescriptions[];

   [Deprecated {"CIM_FCPortStatistics.ErrorFrames"}, Counter, 
       Description (
           "The number of times that a frame was received but no "
           "buffer was available.") ]
   uint64 ReceiveBufferErrors;

   [Deprecated {"CIM_FCPortStatistics.ErrorFrames"}, Counter, 
       Description (
           "The number of times that a frame was received but no "
           "end-to-end credit was available.") ]
   uint64 ReceiveEndErrors;

   [Deprecated {"No value"}, Description (
       "A 'long' timeout value (in milliseconds) for determining "
       "when to reinstate a Recovery_Qualifier. The default value "
       "is 120 seconds (120000 milliseconds). It is typically set "
       "to the ErrorDetectTimeout value + 2*(fabric delay time)."), 
       Units ("MilliSeconds") ]
   uint64 ResourceAllocationTimeout;

   [Deprecated {"No value"}, Description (
       "A 'short' timeout value (in milliseconds) for determining "
       "that an error has occurred. The default value is 10 "
       "seconds (10000 milliseconds)."), 
       Units ("MilliSeconds") ]
   uint64 ErrorDetectTimeout;

   [Deprecated {"No value"}, Counter, Description (
       "Number of Class 1 sequences sent since last reset of the "
       "Device.") ]
   uint64 Class1SequencesSent;

   [Deprecated {"No value"}, Counter, Description (
       "Number of Class 2 sequences sent since last reset of the "
       "Device.") ]
   uint64 Class2SequencesSent;

   [Deprecated {"No value"}, Counter, Description (
       "Number of Class 3 sequences sent since last reset of the "
       "Device.") ]
   uint64 Class3SequencesSent;

   [Deprecated {"No value"}, Counter, Description (
       "Number of Class 4 sequences sent since last reset of the "
       "Device.") ]
   uint64 Class4SequencesSent;

   [Deprecated {"CIM_FCPortStatistics.BytesReceived"}, Counter, 
       Description (
           "Number of octets received by the Adapter when running "
           "Class 2 service.") ]
   uint64 Class2OctetsReceived;

   [Deprecated {"CIM_FCPortStatistics.BytesTransmitted"}, Counter, 
       Description (
           "Number of octets transmitted by the Adapter when running "
           "Class 2 service.") ]
   uint64 Class2OctetsTransmitted;

   [Deprecated {"CIM_FCPortStatistics.PacketsReceived"}, Counter, 
       Description (
           "Number of frames received by the Adapter when running "
           "Class 2 service.") ]
   uint64 Class2FramesReceived;

   [Deprecated {"CIM_FCPortStatistics.PacketsTransmitted"}, Counter, 
       Description (
           "Number of frames transmitted by the Adapter when running "
           "Class 2 service.") ]
   uint64 Class2FramesTransmitted;

   [Deprecated {"No value"}, Counter, Description (
       "Number of frames discarded by the Adapter when running "
       "Class 2 service.") ]
   uint64 Class2DiscardFrames;

   [Deprecated {"CIM_FCPortStatistics.BytesReceived"}, Counter,
       Description (
           "Number of octets received by the Adapter when running "
           "Class 3 service.") ]
   uint64 Class3OctetsReceived;

   [Deprecated {"CIM_FCPortStatistics.BytesTransmitted"}, Counter, 
       Description (
           "Number of octets transmitted by the Adapter when running "
           "Class 3 service.") ]
   uint64 Class3OctetsTransmitted;

   [Deprecated {"CIM_FCPortStatistics.PacketsReceived"}, Counter, 
       Description (
           "Number of frames received by the Adapter when running "
           "Class 3 service.") ]
   uint64 Class3FramesReceived;

   [Deprecated {"CIM_FCPortStatistics.PacketsTransmitted"}, Counter, 
       Description (
           "Number of frames transmitted by the Adapter when running "
           "Class 3 service.") ]
   uint64 Class3FramesTransmitted;

   [Deprecated {"No value"}, Counter, Description (
       "Number of frames discarded by the Adapter when running "
       "Class 3 service.") ]
   uint64 Class3DiscardFrames;

   [Deprecated {"CIM_FCPortStatistics.ErrorFrames"}, Counter, 
       Description (
           "Number of parity errors detected somewhere in the "
           "data path.") ]
   uint64 ParityErrors;

   [Deprecated {"CIM_FCPortStatistics.ErrorFrames"}, Counter,
       Description (
           "Number of Class 1 or 2 frames that are not ACKed "
           "within the time indicated by ErrorDetectTimeout.") ]
   uint64 FrameTimeouts;

   [Deprecated {"CIM_FCPortStatistics.BufferCreditNotProvided"}, 
       Counter, Description (
           "Number of times that the Device has been without a "
           "buffer credit for a time longer than ErrorDetectTimeout.") ]
   uint64 BufferCreditErrors;

   [Deprecated {"CIM_FCPortStatistics.BufferCreditNotReceived"}, 
       Counter, Description (
           "Number of times that the Device has been without an end "
           "credit for a time longer than ErrorDetectTimeout.") ]
   uint64 EndCreditErrors;

   [Deprecated {"CIM_FCPortStatistics.DelimiterErrors"}, Counter, 
       Description ("Number of frames received out of order.") ]
   uint64 OutOfOrderFramesReceived;
};


// ==================================================================
// FibrePort 
// ==================================================================
[Version ("2.7.0"), Deprecated {"CIM_FCPort"}, Description (
    "The use of the FibrePort class is deprecated, since FibreChannel "
    "Adapter has been deprecated in lieu of FCPort.  And, this "
    "class overlaps with FCPort.  The new FCPort class should "
    "be used in lieu of both FibreChannelAdapter and FibrePort. "
    "FibrePort describes the capabilities and management aspects "
    "of a Fibre Channel Port Device.") ]
class CIM_FibrePort : CIM_LogicalPort {

   [Deprecated {"CIM_FCPort.PermanentAddress"}, Description (
       "An address value used to identify the source (S_ID) or "
       "destination (D_ID) of a frame. The FC-SW standard includes a "
       "table of special address identifier values and their "
       "meanings. Consult the FC-SW documentation for additional "
       "information.") ]
   uint32 AddressIdentifier;

   [Deprecated {"No value"}, Description (
       "An array indicating the modes in which the Port can operate. "
       "PortType values describe the role and behavior of the Fibre "
       "Channel entity: \"N\" = Node Port, \"NL\" = Node Port "
       "supporting FC arbitrated loop, \"E\" = Expansion Port "
       "connecting fabric elements (for example, FC switches), "
       "\"F\" = Fabric (element) Port, \"FL\" = Fabric (element) "
       "Port supporting FC arbitrated loop, and \"B\" = Bridge "
       "Port. PortTypes are defined in the ANSI X3 standards. \n\n"
       "A particular mode may be listed multiple times in the "
       "SupportedPortTypes array in order to define that multiple, "
       "unique version levels are supported. Version information is "
       "defined in the PortTypeVersions property. Note that each "
       "entry of the SupportedPortTypes array is related to the entry "
       "in PortTypeVersions that is located at the same index."), 
       ArrayType ("Indexed"), 
       ValueMap {"0", "1", "2", "3", "4", "5", "6", "7"},  
       Values {"Unknown", "N", "NL-Private", "NL-Public", "E", "F", 
           "FL", "B"}, 
       ModelCorrespondence {"CIM_FibrePort.PortTypeVersions"} ]
   uint16 SupportedPortTypes[];

   [Deprecated {"No value"}, Description (
       "Version information for each of the SupportedPortTypes. A "
       "particular PortType (mode) may be listed multiple times in "
       "the SupportedPortTypes array in order to define multiple, "
       "unique version levels. Note that each entry of this array "
       "is related to the entry in SupportedPortTypes that is "
       "located at the same index."), 
       ArrayType ("Indexed"), 
       ModelCorrespondence {"CIM_FibrePort.SupportedPortTypes"} ]
   string PortTypeVersions[];

   [Deprecated {"No value"}, Description (
       "The specific modes currently enabled for the Port. The "
       "values are equal to, or a subset of the values in the Supported"
       "PortTypes array."), 
       ValueMap {"0", "1", "2", "3", "4", "5", "6", "7"},  
       Values {"Unknown", "N", "NL-Private", "NL-Public", "E", "F", 
           "FL", "B"}, 
       ModelCorrespondence {"CIM_FibrePort.SupportedPortTypes", 
           "CIM_FibrePort.EnabledVersions"} ]
   uint16 EnabledPortTypes[];

   [Deprecated {"No value"}, Description (
       "Version information for each of the EnabledPortTypes. A "
       "particular PortType (mode) may be listed multiple times in "
       "the EnabledPortTypes array in order to define multiple, "
       "unique version levels. Note that each entry of this array "
       "is related to the entry in EnabledPortTypes that is located "
       "at the same index."), 
       ArrayType ("Indexed"), 
       ModelCorrespondence {"CIM_FibrePort.EnabledPortTypes"} ]
   string EnabledVersions[];

   [Deprecated {"CIM_FCPort.PortType"}, Description (
       "The specific mode in which the Port is currently running. The "
       "value is one of the entries in the EnabledPortTypes array. The "
       "current port type/mode is dependent on the fibre technology. "
       "For example, in a public loop network, you might indicate a "
       "port type of \"FL\" (value=6) or \"NL\" (value=2)."), 
       ValueMap {"0", "1", "2", "3", "4", "5", "6", "7"},  
       Values {"Unknown", "N", "NL-Private", "NL-Public", "E", "F", 
           "FL", "B"}, 
       ModelCorrespondence {"CIM_FibrePort.EnabledPortTypes", 
           "CIM_FibrePort.CurrentVersion"} ]
   uint16 CurrentPortType;

   [Deprecated {"No value"}, Description (
       "Version information for the CurrentPortType that is active."), 
       ModelCorrespondence {"CIM_FibrePort.CurrentPortType"} ]
   string CurrentVersion;

   [Deprecated {"CIM_FCPort.NetworkAddresses"}, Description (
       "One or more address identifiers that may be recognized by "
       "the Port, in addition to its port-specific identifier. "
       "Multicast or hunt group addresses that are recognized by "
       "the Port would be identified in this array.") ]
   uint32 AliasAddresses[];

   [Deprecated {"CIM_FCPortStatistics.LossOfSignalCounter"}, 
       Counter, Description (
           "Number of times that signal is lost on the Port since "
           "last reset of the Device.") ]
   uint64 LossOfSignalCounter;

   [Deprecated {"CIM_FCPortStatistics.LossOfSyncCounter"}, 
       Counter, Description (
           "Number of times that synchronization is lost on the Port "
           "since last reset of the Device. Synchronization is assumed "
           "lost after a timeout period identified by the Receiver"
           "TransmitterTimeout property.") ]
   uint64 LossOfSyncCounter;

   [Deprecated {"CIM_FCPortStatistics.CRCErrors"}, Counter, 
       Description (
           "Number of times that the CRC in a frame does not match the "
           "CRC computed by the receiver.") ]
   uint64 CRCErrors;

   [Deprecated {"CIM_FCPortStatistics.InvalidTransmissionWords"}, 
       Counter, Description (
           "The number of transmission words that had an 8b10b code "
           "violation in one or more of its characters, had a "
           "K28.5 in its second, third or fourth character positions, "
           "and/or was an ordered set that had an incorrect Beginning "
           "Running Disparity.") ]
   uint64 InvalidTransmissionWords;

   [Deprecated {"CIM_FCPortStatistics.FramesTooShort"}, 
       Counter, Description (
           "The number of frames received that were shorter than 28 "
           "octets. The value of 28 is calculated based on an "
           "assumption of 24 header bytes plus 4 CRC bytes. The "
           "count does not include SOF/EOF bytes which are not data.") ]
   uint64 FramesTooShort;

   [Deprecated {"CIM_FCPortStatistics.FramesTooLong"}, 
       Counter, Description (
           "The number of frames received that were longer than 2140 "
           "octets. The value of 2140 is calculated based on an "
           "assumption of 24 header bytes plus 4 CRC bytes and 2112 "
           "bytes of payload.") ]
   uint64 FramesTooLong;

   [Deprecated {"No value"}, Counter, Description (
       "The number of times that a fill word could not be "
       "inserted, when required. The Elasticity Buffer is defined "
       "in FC-AL. This event might cause data corruption and may "
       "indicate a configuration error or a device out of spec.") ]
   uint64 ElasticityBufferUnderruns;

   [Deprecated {"No value"}, Counter, Description (
       "The number of times that a fill word could not be deleted, "
       "when required. The Elasticity Buffer is defined in FC-AL. "
       "This event might cause data corruption and may indicate a "
       "configuration error or a device out of spec.") ]
   uint64 ElasticityBufferOverruns;

   [Deprecated {"No value"}, Description (
       "Timeout value in milliseconds used to determine when "
       "loss of synchronization has occurred. The typical default "
       "is 100 msec."), 
       Units ("Milliseconds") ]
   uint64 ReceiverTransmitterTimeout;

   [Deprecated {"No value"}, Description (
       "Indication of whether the Port is currently bypassed "
       "(value=2) or not (value=1). A value of 3 (\"Forced Insert\") "
       "describes that the Port is forced active, when it would "
       "otherwise be \"Bypassed\"."), 
       ValueMap {"0", "1", "2", "3"},  
       Values {"Unknown", "Not Bypassed", "Bypassed", 
           "Forced Insert"} ]
   uint16 BypassedState;

   [Deprecated {"No value"}, Description (
       "The type of cabling as sensed by the Port. Not all Fibre"
       "Ports are capable of providing this information. In this "
       "case, a value of 0, \"Unknown\", will be returned. Also, "
       "when single or multi-mode fiber cabling can not be "
       "distinguished, the more general value - 4, \"Fiber-optic\" "
       "- can be specified."), 
       ValueMap {"0", "1", "2", "3", "4", "5", "6"},  
       Values {"Unknown", "Other", "No Media", "Copper/Twinaxial", 
           "Fiber-optic", "Fiber Single Mode", "Fiber Multimode"} ] 
   uint16 ConnectedMedia;
};


// ===================================================================
// FibrePortOnFCAdapter
// ===================================================================
[Association, Version ("2.7.0"), Deprecated {"No value"}, 
    Description (
        "The use of FibrePortOnFCAdapter is deprecated since "
        "both FibrePort and FibreChannelAdapter have been deprecated. "
        "No replacement is needed, since the 2 classes are combined "
        "into a single class.  FibrePortOnFCAdapter associates a "
        "FibrePort with a FibreChannelAdapter.") ]
class CIM_FibrePortOnFCAdapter : CIM_PortOnDevice {

    [Override ("Antecedent"), Deprecated {"No value"},  Max (1), 
        Description (
            "The FibreChannelAdapter that includes the Port.") ]
    CIM_FibreChannelAdapter REF Antecedent;

    [Override ("Dependent"), Max (1), Deprecated {"No value"},  
        Description ("The FibrePort on the Adapter.") ]
    CIM_FibrePort REF Dependent;
};


// ==================================================================
// FibrePortActiveLogin
// ==================================================================
[Association, Version ("2.7.0"), 
    Deprecated {"CIM_ActiveConnection", "CIM_FCPort"},  
    Description (
        "The use of FibrePortActiveLogin is deprecated since "
        "FibrePort is deprecated. Its information is found by "
        "examining the individual FCPorts, and an ActiveConnection "
        "between the FCProtocolEndpoints associated with the ports. "
        "FibrePortActiveLogin indicates that two "
        "FibrePorts are connected via a login and have negotiated "
        "their Class Of Service, frame size and other link "
        "characteristics, as specified by an instance of this class.") ]
class CIM_FibrePortActiveLogin  {

    [Key, Deprecated {"CIM_ActiveConnection.Dependent"}, 
        Description ("The originator of the login.") ]
    CIM_FibrePort REF LoginOriginator;

    [Key, Deprecated {"CIM_ActiveConnection.Antecedent"}, 
        Description ("The responder to the login.") ]
    CIM_FibrePort REF LoginResponder;

    [Key, Deprecated {"CIM_FCPort.ActiveCOS"}, Description (
        "The Fibre Channel Class of Service that is currently running "
        "between the Ports. Since two Ports can be simultaneously "
        "connected at different Classes of Service, this property had "
        "to be part of the object's key and therefore, an instance's "
        "identity."), 
        ValueMap {"0", "1", "2", "3", "4", "5", "6"},  
        Values {"Unknown", "1", "2", "3", "4", "6", "F"}, 
        ModelCorrespondence {"CIM_FibreChannelAdapter.SupportedCOS"},
        MappingStrings {
            "MIF.DMTF|Fibre Channel Bus Port Extensions|001.5"} ]
    uint16 NegotiatedCOS;

   [Deprecated {"CIM_FCPort.ActiveMaximumTransmissionUnit"}, 
       Description (
           "The Fibre Channel frame size, in bytes, that is currently "
           "negotiated between the two Ports."), 
       Units ("Bytes") ]
   uint64 NegotiatedFrameSize;

   [Deprecated {"CIM_FCPort.Speed"}, Description (
       "The speed for communications that is currently negotiated "
       "between the two Ports. Speed is specified in bits per second. "
       "If this information is not available, the property should be "
       "set to 0."), 
       Units ("Bits per Second") ]
   uint64 NegotiatedSpeed;

   [Deprecated {"No value"}, Description (
       "Acknowledgement model negotiated during Port login. For "
       "example, ACK-1 indicates that each frame should be "
       "acknowledged."), 
       ValueMap {"0", "1", "2", "3"},  
       Values {"Unknown", "ACK-0", "ACK-1", "ACK-N"},
       MappingStrings {
           "MIF.DMTF|Fibre Channel Bus Port Extensions|001.6"} ]
   uint16 ACKModel;

   [Deprecated {"No value"}, Description (
       "The buffer-to-buffer model negotiated during Port login. "
       "Either the model defined by the FC-PH standard is used "
       "(value=1, \"Regular\"), or an \"Alternate\" model is "
       "negotiated."), 
       ValueMap {"0", "1", "2"},  
       Values {"Unknown", "Regular", "Alternate"} ]
   uint16 BufferToBufferModel;

   [Deprecated {"No value"}, Description (
       "OriginatorBufferCredit reflects the buffer credit of the "
       "Port defined as the LoginOriginator. It is the number of "
       "frame buffers made available BY the originating Port, TO "
       "the responder Port. Buffer credits are used in point to "
       "point connections, when an NL-Local Port is logged into "
       "another NL-Local Port, and when Nx Ports are logged into "
       "Fx Ports. In other scenarios, this value is undefined."),
       MappingStrings {
           "MIF.DMTF|Fibre Channel Bus Port Extensions|001.3"} ]
   uint64 OriginatorBufferCredit;

   [Deprecated {"No value"}, Description (
       "ResponderBufferCredit reflects the buffer credit of the "
       "Port defined as the LoginResponder. It is the number of "
       "frame buffers made available BY the responder Port, TO "
       "the originating Port. Buffer credits are used in point to "
       "point connections, when an NL-Local Port is logged into "
       "another NL-Local Port, and when Nx Ports are logged into "
       "Fx Ports. In other scenarios, this value is undefined."),
       MappingStrings {
           "MIF.DMTF|Fibre Channel Bus Port Extensions|001.3"} ]
   uint64 ResponderBufferCredit;

   [Deprecated {"No value"}, Description (
       "OriginatorEndCredit reflects the end credit of the Port "
       "defined as the LoginOriginator. It is the number of frame "
       "buffers made available BY the originating Port, TO the "
       "responder Port. End credits are used in point to point "
       "connections, when an NL-Local Port is logged into another "
       "NL-Local Port, and when Nx Ports are logged into remote "
       "Nx Ports. In other scenarios, this value is undefined."),
       MappingStrings {
           "MIF.DMTF|Fibre Channel Bus Port Extensions|001.2"} ]
   uint64 OriginatorEndCredit;

   [Deprecated {"No value"}, Description (
       "ResponderEndCredit reflects the end credit of the Port "
       "defined as the LoginResponder. It is the number of frame "
       "buffers made available BY the responder Port, TO the "
       "originating Port. End credits are used in point to point "
       "connections, when an NL-Local Port is logged into another "
       "NL-Local Port, and when Nx Ports are logged into remote "
       "Nx Ports. In other scenarios, this value is undefined."),
       MappingStrings {
           "MIF.DMTF|Fibre Channel Bus Port Extensions|001.2"} ]
   uint64 ResponderEndCredit;
};


// ==================================================================
// FCAdapterEventCounters 
// ==================================================================
[Version ("2.7.0"), Deprecated {"CIM_FCPortStatistics"}, 
    Description (
        "The use of the FCAdapterEventCounters class is deprecated "
        "since FibreChannelAdapter is deprecated. FCPortStatistics "
        "should be used instead, but redefines the level at which "
        "data is collected. This is why there is no direct translation "
        "of the individual counters between the two classes. This "
        "object describes event counters specific to a "
        "FibreChannelAdapter.") ]
class CIM_FCAdapterEventCounters : CIM_DeviceStatisticalInformation {

    [Deprecated {"No value"}, Counter, 
        Description ("The number of Abort sequence frames received.") ]
    uint64 ABTSFramesReceived;

    [Deprecated {"No value"}, Counter, 
        Description ("The number of Abort sequence frames sent.") ]
    uint64 ABTSFramesSent;

    [Deprecated {"No value"}, Counter, 
        Description ("The number of frames busied by the Fabric.") ]
    uint64 FBSYsReceived;

    [Deprecated {"No value"}, Counter, 
        Description (
            "The number of frames busied by the receiving Node.") ]
    uint64 PBSYsReceived;

    [Deprecated {"No value"}, Counter, Description (
        "The number of frames busied by the Adapter itself.") ]
    uint64 PBSYsSent;

    [Deprecated {"No value"}, Counter, 
        Description ("The number of frames rejected by the Fabric.") ]
    uint64 FRJTsReceived;

    [Deprecated {"No value"}, Counter, Description (
        "The number of frames rejected by the receiving Node.") ]
    uint64 PRJTsReceived;

    [Deprecated {"No value"}, Counter, Description (
        "The number of frames rejected by the Adapter itself.") ]
    uint64 PRJTsSent;

    [Deprecated {"No value"}, Counter, Description (
        "The number of PRLI frames sent where the response was "
        "LS_RJT.") ]
    uint64 PRLIsRejected;

    [Deprecated {"No value"}, Counter, Description (
        "The number of PRLO frames sent where the response was "
        "LS_RJT.") ]
    uint64 PRLOsRejected;

    [Deprecated {"No value"}, Counter, Description (
        "The number of Abort sequence frames sent where the response "
        "was BA_RJT.") ]
    uint64 ABTSFramesRejected;

    [Deprecated {"FCPortStatistics.ResetSelectedStats()"}, Description (
        "Method to reset the Adapter event counters. The method " 
        "takes one parameter as input - an integer indicating which "
        "counter to reset. For this input parameter, 0 indicates all, "
        "1 through 11 indicate a reset of the individual counters. "
        "The method returns 0 if successful, 1 if not supported, and " 
        "any other value if an error occurred. A method is specified "
        "so that the Device's instrumentation, which tabulates "
        "the errors and warnings, can also reset its internal "
        "processing and counters. \n"
        "In a subclass, the set of possible return codes could be "
        "specified, using a ValueMap qualifier on the method. The "
        "strings to which the ValueMap contents are 'translated' "
        "may also be specified in the subclass as a Values "
        "array qualifier.") ]
    uint32 ResetCounter (
        [IN, 
            ValueMap {"0", "1", "2", "3", "4", "5", "6", "7", "8", 
                "9", "10", "11"},
            Values {"All", "ABTSFramesReceived", "ABTSFramesSent", 
                "FBSYReceived", "PBSYReceived", "PBSYSent", 
                "FRJTReceived", "PRJTReceived", "PRJTSent", 
                "PRLIRejected", "PRLORejected", 
                "ABTSFramesRejected"} ]
      uint16 SelectedCounter);
};


// ==================================================================
// FibrePortEventCounters
// ==================================================================
[Version ("2.7.0"), Deprecated {"CIM_FCPortStatistics"}, 
    Description (
        "The use of the FibrePortEventCounters class is deprecated, "
        "since FibrePort is deprecated. FCPortStatistics "
        "should be used instead, but redefines the level at which "
        "data is collected. This is why there is no direct translation "
        "of the individual counters between the two classes. This "
        "object defines error counters specific to a FibrePort.") ]
class CIM_FibrePortEventCounters : CIM_DeviceStatisticalInformation {

    [Deprecated {"No value"}, Counter,  
        Description ("The number of login frames received.") ]
    uint64 PLOGIsReceived;

    [Deprecated {"No value"}, Counter, 
        Description ("The number of login frames sent.") ]
    uint64 PLOGIsSent;

    [Deprecated {"No value"}, Counter, Description (
        "Number of frames received containing 'EOF Abort'.") ]
    uint64 EOFAbortsReceived;

    [Deprecated {"No value"}, Counter, Description (
        "Number of frames transmitted containing 'EOF Abort'.") ]
    uint64 EOFAbortsTransmitted;

    [Deprecated {"No value"}, Counter, Description (
        "The number of logouts received from various targets.") ]
    uint64 PLOGOsReceived;

    [Deprecated {"No value"}, Counter,  
        Description ("The number of logout frames sent.") ]
    uint64 PLOGOsSent;

    [Deprecated {"No value"}, Counter, Description (
        "The number of PLOGI frames sent where the response was "
        "LS_RJT.") ]
    uint64 PLOGIsRejected;
 
    [Deprecated {"No value"}, Counter, Description (
        "The number of PLOGO frames sent where the response was "
        "LS_RJT.") ]
    uint64 PLOGOsRejected;
 
    [Deprecated {"CIM_FCPortStatistics.ResetSelectedStats"}, 
        Description (
        "Method to reset the Port event counters. The method " 
        "takes one parameter as input - an integer indicating which "
        "counter to reset. For this input parameter, 0 indicates all, "
        "1 through 8 indicate a reset of the individual counters. "
        "The method returns 0 if successful, 1 if not supported, and " 
        "any other value if an error occurred. A method is specified "
        "so that the Device's instrumentation, which tabulates "
        "the errors and warnings, can also reset its internal "
        "processing and counters. \n"
        "In a subclass, the set of possible return codes could be "
        "specified, using a ValueMap qualifier on the method. The "
        "strings to which the ValueMap contents are 'translated' "
        "may also be specified in the subclass as a Values "
        "array qualifier.") ]
    uint32 ResetCounter (
        [IN, 
            ValueMap {"0", "1", "2", "3", "4", "5", "6", "7", "8"},
            Values {"All", "PLOGIsReceived", "PLOGIsSent", 
                "EOFAbortsReceived", "EOFAbortsTransmitted", 
                "PLOGOsReceived", "PLOGOsSent", "PLOGIsRejected", 
                "PLOGOsRejected"} ] 
       uint16 SelectedCounter);
};


// ===================================================================
// end of file
// ===================================================================
