-- MODULE NAME: ITSANM.mib
--
-- IBM TotalStorage Productivity Center Fabric Manager MIBs Version 2.1
--
-- This text file defines several OIDs which are used
-- to depict an IBM TotalStorage Productivity Center Fabric Manager event.  The event
-- is sent out by Event Services as an SNMP trap. Each SNMP
-- trap contains ...x... objects.

ITSANM-MIB DEFINITIONS ::= BEGIN
IMPORTS
    enterprises
         FROM RFC1155-SMI
    DisplayString
         FROM RFC1213-MIB
    OBJECT-TYPE
         FROM RFC-1212;

--   MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
--        FROM SNMPv1-CONF;

--   IBMProd, IBMMod
--        FROM IBM-GLOBAL-REG;

-- IBM Corporation info.
ibm                             OBJECT IDENTIFIER ::= { enterprises 2 }
ibmProd                         OBJECT IDENTIFIER ::= { ibm 6 }
--Tivoli San Management info.
tivoliSANManagement             OBJECT IDENTIFIER  ::= { ibmProd 173 }
btaVariables                    OBJECT IDENTIFIER  ::= { tivoliSANManagement 1 }
btaNetworkManager               OBJECT IDENTIFIER  ::= { tivoliSANManagement 3 }
btaCommon                       OBJECT IDENTIFIER  ::= { tivoliSANManagement 5 }
btaNetviewDisplaySymbols        OBJECT IDENTIFIER  ::= { tivoliSANManagement 6 }
btaTryAndBuyLicense             OBJECT IDENTIFIER  ::= { tivoliSANManagement 7 }


-- *******************************************************************
-- btaVariables
-- *******************************************************************
btatrapDescription OBJECT-TYPE
        SYNTAX DisplayString (SIZE(1..127))
        ACCESS read-only
        STATUS mandatory
        DESCRIPTION
          "Description of this trap"
        ::= { btaVariables 1}

btahostName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The host associated with the trap"
        ::= { btaVariables 2 }

btadeviceClass OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The device class"
        ::= { btaVariables 7 }

btaWWN OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The World Wide Name"
        ::= { btaVariables 8 }

btamessagePrefix OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The IBM TotalStorage Productivity Center message prefix for Fabric"
        ::= { btaVariables 9 }

btalicenseDaysRemaining OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The number of days"
        ::= { btaVariables 10 }

btapeEntityType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Entity Event entity type"
        ::= { btaVariables 22 }

btapeHighLevelDeviceUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Entity Event high level device unique Id"
        ::= { btaVariables 23 }

btapeHighLevelDeviceLabel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Entity Event high level device label"
        ::= { btaVariables 24 }

btapeHighLevelDeviceType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Entity Event high level device type"
        ::= { btaVariables 25 }

btapeState OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Entity Event state"
        ::= { btaVariables 26 }

btapeEventType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Entity Event event type"
        ::= { btaVariables 27 }

btaprEntityType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event entity type"
        ::= { btaVariables 28 }

btaprUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event unique Id"
        ::= { btaVariables 29 }

btaprToObjectHighLevelDeviceUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event to object high level device unique Id"
        ::= { btaVariables 30 }

btaprToObjectHighLevelDeviceLabel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event to object high level device label"
        ::= { btaVariables 31 }

btaprToObjectHighLevelDeviceType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event to object high level device type"
        ::= { btaVariables 32 }

btaprFromObjectHighLevelDeviceUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event from object high level device unique Id"
        ::= { btaVariables 33 }

btaprFromObjectHighLevelDeviceLabel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event from object high level device label"
        ::= { btaVariables 34 }

btaprFromObjectHighLevelDeviceType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event from object high level device type"
        ::= { btaVariables 35 }

btaprState OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event state"
        ::= { btaVariables 36 }

btaprEventType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Physical Relationship Event event type"
        ::= { btaVariables 37 }

btaleEntityType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Entity Event entity type"
        ::= { btaVariables 38 }

btaleUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Entity Event unique Id"
        ::= { btaVariables 39 }

btaleLabel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Entity Event label"
        ::= { btaVariables 40 }

btaleType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Entity Event type"
        ::= { btaVariables 41 }

btaleState OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Entity Event state"
        ::= { btaVariables 42 }

btaleEventType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Entity Event event type"
        ::= { btaVariables 43 }

btalrEntityType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event entity type"
        ::= { btaVariables 44 }

btalrUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event unique Id"
        ::= { btaVariables 45 }

btalrToObjectUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event to object unique Id"
        ::= { btaVariables 46 }

btalrToObjectLabel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event to object label"
        ::= { btaVariables 47 }

btalrToObjectType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event to object type"
        ::= { btaVariables 48 }

btalrFromObjectUniqueId OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event from object unique Id"
        ::= { btaVariables 49 }

btalrFromObjectLabel OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event from object label"
        ::= { btaVariables 50 }

btalrFromObjectType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event from object type"
        ::= { btaVariables 51 }

btalrState OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event state"
        ::= { btaVariables 52 }

btalrEventType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Logical Relationship Event event type"
        ::= { btaVariables 53 }

btaactionPerformed OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Fabric Manager Status Event action performed"
        ::= { btaVariables 54 }

btasrSANName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The SAN Region event SAN name"
        ::= { btaVariables 55 }

btasrZoneName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The SAN Region event Zone name"
        ::= { btaVariables 56 }

btasrState OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The SAN Region event state"
        ::= { btaVariables 57 }

btasrEventType OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The SAN Region event event type"
        ::= { btaVariables 58 }

btaserviceName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Service Event service name"
        ::= { btaVariables 59 }

btaserviceState OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The Service Event service state"
        ::= { btaVariables 60 }

btasrActive OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "Active ZoneSet indicator"
        ::= { btaVariables 61 }

btasrZSetName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The name of the ZoneSet"
        ::= { btaVariables 62 }

-- Added for operational status 08/25/05
btaOldStatus OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The old value of the Operational status"
        ::= { btaVariables 63 }

btaNewStatus OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The new value of the operational status change."
        ::= { btaVariables 64 }

-- Added for attributes 08/25/05
btaAtributeName OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The name of the attribute"
        ::= { btaVariables 65 }

btaOldValue OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The old value of the given attribute name."
        ::= { btaVariables 66 }

btaNewValue OBJECT-TYPE
        SYNTAX  DisplayString (SIZE(1..127))
        ACCESS  read-only
        STATUS  mandatory
        DESCRIPTION
          "The new value of the given value"
        ::= { btaVariables 67 }

-- *******************************************************************
-- btaNetworkManager Traps
-- *******************************************************************
-- **
-- * A more "standard" way of determining the SNMP Trap Specific value is being
-- * used in 1.2,  All SNMP Trap Specific values should be greater than 100. All
-- * traps for severe problems should be odd number values > 100, and all other
-- * traps should be even number values > 100.
-- **
-- High severity traps = 101, and 103
--
-- Less serious traps  = 102, 104, 106, 108, 110, 112, and 114
--
--	
--
-- Enterprise Names	                     OIDs	                    Trap Names	                        Trap 
-- ---------------------------------     ------------------------   -----------------------------       ----
-- btaNetworkManagerPhysicalEntity 	     1.3.6.1.4.1.2.6.173.3.30   btaMissingPhysicalDeviceEvent	     101
--		                                                            btaNewPhysicalDeviceEvent 		     104
--		                                                            btaNormalPhysicalDeviceEvent 		 112
--		                                                            btaModifiedPhysicalAttributeEvent	 102
--			
-- btaNetworkManagerPhysicalRelationship 1.3.6.1.4.1.2.6.173.3.31	btaMissingPhysicalRelationshipEvent	 103
--		                                                            btaNewPhysicalRelationshipEvent		 106
--		                                                            btaNormalPhysicalRelationshipEvent	 114
--			
-- btaNetworkManagerLogicalEntity	     1.3.6.1.4.1.2.6.173.3.32	btaMissingLogicalDeviceEvent		 101
--		                                                            btaNewLogicalDeviceEvent		     104
--		                                                            btaNormalLogicalDeviceEvent		     112
--		                                                            btaModifiedLogicalAttributeEvent	 102
--			
-- btaNetworkManagerLogicalRelationship	 1.3.6.1.4.1.2.6.173.3.33	btaMissingLogicalRelationshipEvent	 103
--		                                                            btaNewLogicalRelationshipEvent		 106
--		                                                            btaNormalLogicalRelationshipEvent	 114
--			
-- btaNetworkManagerSANManagerStatus	 1.3.6.1.4.1.2.6.173.3.34	btaClearChangesDoneEvent		     108
--		                                                            btaModelUpdatedEvent	             110
--			
-- btaNetworkManagerSANRegion	         1.3.6.1.4.1.2.6.173.3.35	btaMissingSANRegionDeviceEvent		 101
--									                                btaMissingSANRegionRelationshipEvent 103
--									                                btaNewSANRegionDeviceEvent		     104
--									                                btaNewSANRegionRelationshipEvent	 106
--									                                btaNormalSANRegionDeviceEvent		 112
--									                                btaNormalSANRegionRelationshipEvent	 114
--									                                btaModifiedSANRegionAttributeEvent	 102
--			
-- btaNetworkManagerService	             1.3.6.1.4.1.2.6.173.3.36   btaServiceStartupEvent                 1
--                                                                  btaServiceShutdownEvent                2		
                                                            
btaNetworkManagerPhysicalEntity          OBJECT IDENTIFIER ::= { btaNetworkManager 30 }
btaNetworkManagerPhysicalRelationship    OBJECT IDENTIFIER ::= { btaNetworkManager 31 }
btaNetworkManagerLogicalEntity           OBJECT IDENTIFIER ::= { btaNetworkManager 32 }
btaNetworkManagerLogicalRelationship     OBJECT IDENTIFIER ::= { btaNetworkManager 33 }
btaNetworkManagerSANManagerStatus        OBJECT IDENTIFIER ::= { btaNetworkManager 34 }
btaNetworkManagerSANRegion               OBJECT IDENTIFIER ::= { btaNetworkManager 35 }
btaNetworkManagerService                 OBJECT IDENTIFIER ::= { btaNetworkManager 36 }
                                                            
                                                            
-- *******************************************************************
-- Missing Device Traps
-- *******************************************************************
btaMissingPhysicalDeviceEvent    TRAP-TYPE                     
      ENTERPRISE         btaNetworkManagerPhysicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btapeEntityType,
                           btapeHighLevelDeviceUniqueId,
                           btapeHighLevelDeviceLabel,
                           btapeHighLevelDevicecType,
                           btapeState,
                           btapeEventType  }
      DESCRIPTION       "A Missing Physical Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaMissingPhysicalDeviceEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtapeEntityType=$5;\nbtapeHighLevelDeviceUniqueId=$6;\nbtapeHighLevelDeviceLabel=$7;"
      --#SUMMARY   "btapeHighLevelDeviceType=$8;\nbtapeState=$9;\nbtapeEventType=$10;"
      --#SEVERITY  CRITICAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  101

btaMissingLogicalDeviceEvent    TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaleUniqueId,
                           btaleEntityType,
                           btaleLabel,
                           btaleType,
                           btaleState,
                           btaleEventType  }
      DESCRIPTION       "A Missing Logical Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaMissingLogicalDeviceEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaleUniqueId=$5;\nbtaleEntityType=$6;\nbtaleLabel=$7;\nbtaleType=$8;\nbtaleState=$9;\nbtaleEventType=$10;"
      --#SEVERITY  CRITICAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  101

btaMissingSANRegionDeviceEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName  }                           
      DESCRIPTION       "A Missing SAN Region Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaMissingSANRegionDeviceEvent trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  CRITICAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  101

                                       
-- *******************************************************************
-- Missing Relationship Traps
-- *******************************************************************
btaMissingPhysicalRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerPhysicalRelationship
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaprUniqueId,
                           btaprEntityType,
                           btaprToObjectHighLevelDeviceUniqueId,
                           btaprToObjectHighLevelDeviceLabel,
                           btaprToObjectHighLevelDeviceType,
                           btaprFromObjectHighLevelDeviceUniqueId,
                           btaprFromObjectHighLevelDeviceLabel,
                           btaprFromObjectHighLevelDeviceType,
                           btaprState,
                           btaprEventType  }
      DESCRIPTION       "A Missing Physical Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaMissingPhysicalRelationshipEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaprUniqueId=$5;\nbtaprEntityType=$6;\nbtaprToObjectHighLevelDeviceUniqueId=$7;"
      --#SUMMARY   "btaprToObjectHighLevelDeviceLabel=$8;\nbtaprToObjectHighLevelDeviceType=$9;\nbtaprFromObjectHighLevelDeviceUniqueId=$10;\nbtaprFromObjectHighLevelDeviceLabel=$11;\nbtaprFromObjectHighLevelDeviceType=$12;\nbtaprState=$13;\nbtaprEventType=$14;"
      --#SEVERITY  CRITICAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  103

btaMissingLogicalRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalRelationship
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btalrUniqueId,
                           btalrEntityType,
                           btalrToObjectUniqueId,
                           btalrToObjectLabel,
                           btalrToObjectType,
                           btalrFromObjectUniqueId,
                           btalrFromObjectLabel,
                           btalrFromObjectType,
                           btalrState,
                           btalrEventType  }
      DESCRIPTION       "A Missing Logical Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaMissingLogicalRelationshipEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtalrUniqueId=$5;\nbtalrEntityType=$6;\nbtalrToObjectUniqueId=$7;\nbtalrToObjectLabel=$8;"
      --#SUMMARY   "btalrToObjectType=$9;\nbtalrFromObjectUniqueId=$10;\nbtalrFromObjectLabel=$11;\nbtalrFromObjectType=$12;\nbtalrState=$13;\nbtalrEventType=$14;"
      --#SEVERITY  CRITICAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  103

btaMissingSANRegionRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName  }                           
      DESCRIPTION       "A Missing SAN Region Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaMissingSANRegionRelationshipEvent trap from $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  CRITICAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  103



-- *******************************************************************
-- New Device Traps
-- *******************************************************************
btaNewPhysicalDeviceEvent        TRAP-TYPE					
      ENTERPRISE         btaNetworkManagerPhysicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btapeEntityType,
                           btapeHighLevelDeviceUniqueId,
                           btapeHighLevelDeviceLabel,
                           btapeHighLevelDeviceType,
                           btapeState,
                           btapeEventType  }
      DESCRIPTION       "A New Physical Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNewPhysicalDeviceEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtapeEntityType=$5;\nbtapeHighLevelDeviceUniqueId=$6;\nbtapeHighLevelDeviceLabel=$7;"
      --#SUMMARY   "btapeHighLevelDeviceType=$8;\nbtapeState=$9;\nbtapeEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  104

btaNewLogicalDeviceEvent    TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaleUniqueId,
                           btaleEntityType,
                           btaleLabel,
                           btaleType,
                           btaleState,
                           btaleEventType  }
      DESCRIPTION       "A New Logical Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNewLogicalDeviceEvent trap from $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaleUniqueId=$5;\nbtaleEntityType=$6;\nbtaleLabel=$7;\nbtaleType=$8;\nbtaleState=$9;\nbtaleEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL  
      ::=  104

btaNewSANRegionDeviceEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName  }
      DESCRIPTION       "A New SAN Region Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNewSANRegionDeviceEvent trap from $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  WARNING
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  104


                                       
-- *******************************************************************
-- New Relationship Traps
-- *******************************************************************
btaNewPhysicalRelationshipEvent  TRAP-TYPE
      ENTERPRISE         btaNetworkManagerPhysicalRelationship
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaprUniqueId,
                           btaprEntityType,
                           btaprToObjectHighLevelDeviceUniqueId,
                           btaprToObjectHighLevelDeviceLabel,
                           btaprToObjectHighLevelDeviceType,
                           btaprFromObjectHighLevelDeviceUniqueId,
                           btaprFromObjectHighLevelDeviceLabel,
                           btaprFromObjectHighLevelDeviceType,
                           btaprState,
                           btaprEventType  }
      DESCRIPTION       "A New Physical Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNewPhysicalRelationshipEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaprUniqueId=$5;\nbtaprEntityType=$6;\nbtaprToObjectHighLevelDeviceUniqueId=$7;"
      --#SUMMARY   "btaprToObjectHighLevelDeviceLabel=$8;\nbtaprToObjectHighLevelDeviceType=$9;\nbtaprFromObjectHighLevelDeviceUniqueId=$10;\nbtaprFromObjectHighLevelDeviceLabel=$11;\nbtaprFromObjectHighLevelDeviceType=$12;\nbtaprState=$13;\nbtaprEventType=$14;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  106

btaNewLogicalRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalRelationship
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btalrUniqueId,
                           btalrEntityType,
                           btalrToObjectUniqueId,
                           btalrToObjectLabel,
                           btalrToObjectType,
                           btalrFromObjectUniqueId,
                           btalrFromObjectLabel,
                           btalrFromObjectType,
                           btalrState,
                           btalrEventType  }
      DESCRIPTION       "A New Logical Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNewLogicalRelationshipEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtalrUniqueId=$5;\nbtalrEntityType=$6;\nbtalrToObjectUniqueId=$7;\nbtalrToObjectLabel=$8;"
      --#SUMMARY   "btalrToObjectType=$9;\nbtalrFromObjectUniqueId=$10;\nbtalrFromObjectLabel=$11;\nbtalrFromObjectType=$12;\nbtalrState=$13;\nbtalrEventType=$14;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  106

btaNewSANRegionRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName  }                           
      DESCRIPTION       "A New SAN Region Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNewSANRegionRelationshipEvent trap from $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  106



-- *******************************************************************
-- Normal Device Traps
-- *******************************************************************
btaNormalPhysicalDeviceEvent     TRAP-TYPE				
      ENTERPRISE         btaNetworkManagerPhysicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btapeEntityType,
                           btapeHighLevelDeviceUniqueId,
                           btapeHighLevelDeviceLabel,
                           btapeHighLevelDeviceType,
                           btapeState,
                           btapeEventType  }
      DESCRIPTION       "A Normal Physical Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNormalPhysicalDeviceEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtapeEntityType=$5;\nbtapeHighLevelDeviceUniqueId=$6;\nbtapeHighLevelDeviceLabel=$7;"
      --#SUMMARY   "btapeHighLevelDeviceType=$8;\nbtapeState=$9;\nbtapeEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  112

btaNormalLogicalDeviceEvent    TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaleUniqueId,
                           btaleEntityType,
                           btaleLabel,
                           btaleType,
                           btaleState,
                           btaleEventType  }
      DESCRIPTION       "A Normal Logical Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNormalLogicalDeviceEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaleUniqueId=$5;\nbtaleEntityType=$6;\nbtaleLabel=$7;\nbtaleType=$8;\nbtaleState=$9;\nbtaleEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  112

btaNormalSANRegionDeviceEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName  }                             
      DESCRIPTION       "A Normal SAN Region Device Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNormalSANRegionDeviceEvent trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  WARNING
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  112



-- *******************************************************************
-- Normal Relationship Traps
-- *******************************************************************
btaNormalPhysicalRelationshipEvent  TRAP-TYPE
      ENTERPRISE         btaNetworkManagerPhysicalRelationship
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaprUniqueId,
                           btaprEntityType,
                           btaprToObjectHighLevelDeviceUniqueId,
                           btaprToObjectHighLevelDeviceLabel,
                           btaprToObjectHighLevelDeviceType,
                           btaprFromObjectHighLevelDeviceUniqueId,
                           btaprFromObjectHighLevelDeviceLabel,
                           btaprFromObjectHighLevelDeviceType,
                           btaprState,
                           btaprEventType  }
      DESCRIPTION       "A Normal Physical Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNormalPhysicalRelationshipEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaprUniqueId=$5;\nbtaprEntityType=$6;\nbtaprToObjectHighLevelDeviceUniqueId=$7;"
      --#SUMMARY   "btaprToObjectHighLevelDeviceLabel=$8;\nbtaprToObjectHighLevelDeviceType=$9;\nbtaprFromObjectHighLevelDeviceUniqueId=$10;\nbtaprFromObjectHighLevelDeviceLabel=$11;\nbtaprFromObjectHighLevelDeviceType=$12;\nbtaprState=$13;\nbtaprEventType=$14;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  114

btaNormalLogicalRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalRelationship
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btalrUniqueId,
                           btalrEntityType,
                           btalrToObjectUniqueId,
                           btalrToObjectLabel,
                           btalrToObjectType,
                           btalrFromObjectUniqueId,
                           btalrFromObjectLabel,
                           btalrFromObjectType,
                           btalrState,
                           btalrEventType  }
      DESCRIPTION       "A Normal Logical Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNormalLogicalRelationshipEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtalrUniqueId=$5;\nbtalrEntityType=$6;\nbtalrToObjectUniqueId=$7;\nbtalrToObjectLabel=$8;"
      --#SUMMARY   "btalrToObjectType=$9;\nbtalrFromObjectUniqueId=$10;\nbtalrFromObjectLabel=$11;\nbtalrFromObjectType=$12;\nbtalrState=$13;\nbtalrEventType=$14;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  114

btaNormalSANRegionRelationshipEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName  }                           
      DESCRIPTION       "A Normal SAN Region Relationship Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaNormalSANRegionRelationshipEvent trap from $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  114



-- *******************************************************************
-- Modified Attribute Traps
-- *******************************************************************
btaModifiedPhysicalAttributeEvent  TRAP-TYPE        		
      ENTERPRISE         btaNetworkManagerPhysicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btapeEntityType,
                           btapeHighLevelDeviceUniqueId,
                           btapeHighLevelDeviceLabel,
                           btapeHighLevelDeviceType,
                           btapeState,
                           btapeEventType,
                           btaAttributeName,
                           btaOldValue,
                           btaNewValue}   
                           
      DESCRIPTION       "A Modified Physical Attribute Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaModifiedPhysicalAttributeEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtapeEntityType=$5;\nbtapeHighLevelDeviceUniqueId=$6;\nbtapeHighLevelDeviceLabel=$7;"
      --#SUMMARY   "btapeHighLevelDeviceType=$8;\nbtapeState=$9;\nbtapeEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  102

btaModifiedLogicalAttributeEvent    TRAP-TYPE
      ENTERPRISE         btaNetworkManagerLogicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btaleUniqueId,
                           btaleEntityType,
                           btaleLabel,
                           btaleType,
                           btaleState,
                           btaleEventType,
                           btaAttributeName,
                           btaOldValue,
                           btaNewValue }
      DESCRIPTION       "A Modified Logical Attribute Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaModifiedLogicalAttributeEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtaleUniqueId=$5;\nbtaleEntityType=$6;\nbtaleLabel=$7;\nbtaleType=$8;\nbtaleState=$9;"
      --#SUMMARY   "btapeEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  102

btaModifiedSANRegionAttributeEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName,
                           btaAttributeName,
                           btaOldValue,
                           btaNewValue }                                                      
      DESCRIPTION       "A Modified SAN Region Attribute Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaModifiedSANRegionAttributeEvent trap from $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  102


-- *******************************************************************
-- Operational status change Traps added 8/25/05
-- *******************************************************************
btaPEOperationalStatusChangeEvent  TRAP-TYPE        		
      ENTERPRISE         btaNetworkManagerPhysicalEntity
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btapeEntityType,
                           btapeHighLevelDeviceUniqueId,
                           btapeHighLevelDeviceLabel,
                           btapeHighLevelDeviceType,
                           btapeState,
                           btapeEventType,
                           btaOldStatus,
                           btaNewStatus}   
                           
      DESCRIPTION       "A Modified Physical Attribute Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaModifiedPhysicalAttributeEvent trap from enterprise $E, with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtapeEntityType=$5;\nbtapeHighLevelDeviceUniqueId=$6;\nbtapeHighLevelDeviceLabel=$7;"
      --#SUMMARY   "btapeHighLevelDeviceType=$8;\nbtapeState=$9;\nbtapeEventType=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  116

btaSROperationalStatusChangeEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANRegion
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btadeviceClass,
                           btaWWN,
                           btasrSANName,
                           btasrZoneName,
                           btasrState,
                           btasrEventType,
                           btasrActive,
                           btasrZSetName,
                           btaOldStatus,
                           btaNewStatus }                                                      
      DESCRIPTION       "A Modified SAN Region Attribute Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaModifiedSANRegionAttributeEvent trap from $E with $# args:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaDeviceClass=$3;\nbtaWWN=$4;\nbtasrSANName$5;\nbtasrZoneName=$6;\nbtasrState=$7;\nbtasrEventType=$8;\nbtasrActive=$9;\nbtasrZSetName=$10;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  116
 

-- *******************************************************************
-- Clear Changes Trap
-- *******************************************************************
btaClearChangesDoneEvent  TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANManagerStatus
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btaactionPerformed  }
      DESCRIPTION       "A Clear Changes Done Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaClearChangesDoneEvent trap from enterprise $E with $# arg:\nbtatrapDescription=$1;\nbtaMessagePrefix=$2;\nbtaactionPerformed=$3;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  108


                                 
-- *******************************************************************
-- Model Updated Trap
-- *******************************************************************
btaModelUpdatedEvent     TRAP-TYPE
      ENTERPRISE         btaNetworkManagerSANManagerStatus
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btaactionPerformed  }
      DESCRIPTION       "A Model Updated Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaModelUpdatedEvent trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtamessagePrefix=$2;\nbtaactionPerformed=$3;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  110


                                 
-- *******************************************************************
-- Service Startup Trap
-- *******************************************************************
btaServiceStartupEvent   TRAP-TYPE
      ENTERPRISE         btaNetworkManagerService
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btaserviceName,
                           btaserviceState }
      DESCRIPTION       "A Service Startup Event."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaServiceStartupEvent trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtamessagePrefix=$2;\nbtaserviceName=$3;\nbtaserviceState=$4;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  1

                                 
-- *******************************************************************
-- Service Shutdown Trap
-- *******************************************************************
btaServiceShutdownEvent  TRAP-TYPE
      ENTERPRISE         btaNetworkManagerService
      VARIABLES          { btatrapDescription,
                           btamessagePrefix,
                           btaserviceName,
                           btaserviceState }
      DESCRIPTION       "A Service Shutdown."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaServiceShutdownEvent trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtamessagePrefix=$2;\nbtaserviceName=$3;\nbtaserviceState=$4;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  2



-- *******************************************************************
-- The following btaCommon and btaTryAndBuyLicense traps are legacy
-- traps from ITSANM 1.1 which are still supported in ITSANM 1.2 
-- *******************************************************************
-- *******************************************************************
-- btaCommon Traps
-- *******************************************************************        
btaServiceStartup       OBJECT IDENTIFIER ::= { btaCommon 1 }
btaServiceStartup_      TRAP-TYPE
      ENTERPRISE        btaServiceStartup
      VARIABLES         { btatrapDescription,
                          btamessagePrefix,
                          btaobjectName,
                          btahostName }
      DESCRIPTION       "An IBM TotalStorage Productivity Center service has completed startup for Fabric."     
      --#SOURCE_ID "a"
      --#SUMMARY   "btaServiceStartup_ trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtamessagePrefix=$2;\nbtaobjectName=$3;\nbtahostName=$4;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  1


btaServiceShutdown       OBJECT IDENTIFIER ::= { btaCommon 2 }
btaServiceShutdown_      TRAP-TYPE
      ENTERPRISE        btaServiceShutdown
      VARIABLES         { btatrapDescription,
                          btamessagePrefix,
                          btaobjectName,
                          btahostName }
      DESCRIPTION       "An IBM TotalStorage Productivity Center service is shutting down for Fabric."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaServiceShutdown_ trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtamessagePrefix=$2;\nbtaobjectName=$3;\nbtahostName=$4;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::=  2


-- *******************************************************************
-- btaTryAndBuyLicense Trap
-- *******************************************************************
btaLicense              OBJECT IDENTIFIER ::= { btaTryAndBuyLicense 1 }
btaLicense_             TRAP-TYPE
       ENTERPRISE       btaLicense
       VARIABLES        { btatrapDescription,
                          btamessagePrefix,
                          btalicenseDaysRemaining }
      DESCRIPTION       "# day(s) left on Try and Buy License."
      --#SOURCE_ID "a"
      --#SUMMARY   "btaLicense_ trap from enterprise $E with $# args:\nbtatrapDescription=$1;\nbtamessagePrefix=$2;\nbtalicenseDaysRemaining=$3;"
      --#SEVERITY  INFORMATIONAL
      --#CATEGORY  "Status Events"
      --#STATE     OPERATIONAL
      ::= 1 
END
