// ===================================================================
// Title:       Device Infiniband 2.7
// Filename:    Device27_IB.mof
// Version:     2.7.0
// Release:     Final
// Date:        03/31/03
// ===================================================================
// Copyright 2000-2003 Distributed Management Task Force, Inc. (DMTF).
// All rights reserved.  
// DMTF is a not-for-profit association of industry members dedicated 
// to promoting enterprise and systems management and interoperability. 
// DMTF specifications and documents may be reproduced for uses
// consistent with this purpose by members and non-members, 
// provided that correct attribution is given. 
// As DMTF specifications may be revised from time to time, 
// the particular version and release date should always be noted.
//
// Implementation of certain elements of this standard or proposed 
// standard may be subject to third party patent rights, including 
// provisional patent rights (herein "patent rights"). DMTF makes 
// no representations to users of the standard as to the existence 
// of such rights, and is not responsible to recognize, disclose, or
// identify any or all such third party patent right, owners or 
// claimants, nor for any incomplete or inaccurate identification or 
// disclosure of such rights, owners or claimants. DMTF shall have no 
// liability to any party, in any manner or circumstance, under any 
// legal theory whatsoever, for failure to recognize, disclose, or 
// identify any such third party patent rights, or for such party's
// reliance on the standard or incorporation thereof in its product, 
// protocols or testing procedures. DMTF shall have no liability to 
// any party implementing such standard, whether such implementation 
// is foreseeable or not, nor to any patent owner or claimant, and shall 
// have no liability or responsibility for costs or losses incurred if 
// a standard is withdrawn or modified after publication, and shall be
// indemnified and held harmless by any party implementing the 
// standard from any and all claims of infringement by a patent owner 
// for such implementations.
//
// For information about patents held by third-parties which have 
// notified the DMTF that, in their opinion, such patent may relate to 
// or impact implementations of DMTF standards, visit 
// http://www.dmtf.org/about/policies/disclosures.php.
// ===================================================================
// Description: The Device Model extends the management concepts that
//              are related to LogicalDevices. This file defines the 
//              classes to manage Infiniband devices.
//
//              The object classes below are listed in an order that
//              avoids forward references. Required objects, defined 
//              by other working groups, are omitted.
// ==================================================================
// Change Log for v2.7 Final
// CR962 - Fix the overlapping values defined for PortTypes.
// CR971 - Remove the experimental IB class definitions so they can 
//         remain experimental in 2.8
//
// Change Log for v2.7
// CR631 - Add IBPortStatistics
// CR633 - Add IBPort
// CR783 - Add IBPortController
//       - Modify IBPort
// ================================================================== 

#pragma locale ("en_US")


// ===================================================================
// IBSubnetManager
// =================================================================== 
[Version("2.7.0"), Description (
    "An Infiniband Subnet Manager (SM) is an entity responsible "
    "for configuring and managing an IB subnet. It uses Subnet "
    "Management Agents (SMA) to access and manage individual "
    "nodes. The SM is hosted in the context of a specific "
    "computer system (i.e., hosted by an instance of "
    "UnitaryComputerSystem), as described by the HostedService "
    "association. Note that there may be multiple SMs operating "
    "in a subnet, but only the elected master is allowed to "
    "perform configuration functions.") ]
class CIM_IBSubnetManager : CIM_Service {
    
    [Description (
        "Administratively assigned priority for this SM, used to "
        "establish the master. A higher number indicates a higher "
        "priority and likelihood of becoming the master. The property "
        "value can be reset by the master SM."),
        Write,
        MappingStrings {"MAD.IBTA | SMInfo | Priority"} ]
    uint8 Priority;
    
    [Description (
        "Enumerated value that indicates the Subnet Manager's State. "
        "The values are fairly self-explanatory except for \"Not "
        "Active\". This value indicates that the SM is available to "
        "participate in the subnet, but has not been given "
        "permission.  A value \"Unknown\" (0) is also defined."),
        ValueMap {"0", "1", "2", "3", "4"},
        Values {"Unknown", "Not Active", "Discovering", "Standby", 
            "Master"},
        MappingStrings {"MAD.IBTA | SMInfo | SMState"} ]
    uint16 State;
};


// ===================================================================
// end of file
// ===================================================================
